Release 12.2 - xst M.63c (nt)
Copyright (c) 1995-2010 Xilinx, Inc.  All rights reserved.
--> Parameter TMPDIR set to xst/projnav.tmp


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.20 secs
 
--> Parameter xsthdpdir set to xst


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.20 secs
 
--> Reading design: top.prj

TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Compilation
  3) Design Hierarchy Analysis
  4) HDL Analysis
  5) HDL Synthesis
     5.1) HDL Synthesis Report
  6) Advanced HDL Synthesis
     6.1) Advanced HDL Synthesis Report
  7) Low Level Synthesis
  8) Partition Report
  9) Final Report
	9.1) Device utilization summary
	9.2) Partition Resource Summary
	9.3) TIMING REPORT


=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input File Name                    : "top.prj"
Input Format                       : mixed
Ignore Synthesis Constraint File   : NO

---- Target Parameters
Output File Name                   : "top"
Output Format                      : NGC
Target Device                      : xc3s1200e-4-fg320

---- Source Options
Top Module Name                    : top
Automatic FSM Extraction           : YES
FSM Encoding Algorithm             : Auto
Safe Implementation                : No
FSM Style                          : LUT
RAM Extraction                     : Yes
RAM Style                          : Auto
ROM Extraction                     : Yes
Mux Style                          : Auto
Decoder Extraction                 : YES
Priority Encoder Extraction        : Yes
Shift Register Extraction          : YES
Logical Shifter Extraction         : YES
XOR Collapsing                     : YES
ROM Style                          : Auto
Mux Extraction                     : Yes
Resource Sharing                   : YES
Asynchronous To Synchronous        : NO
Multiplier Style                   : Auto
Automatic Register Balancing       : No

---- Target Options
Add IO Buffers                     : YES
Global Maximum Fanout              : 500
Add Generic Clock Buffer(BUFG)     : 24
Register Duplication               : YES
Slice Packing                      : YES
Optimize Instantiated Primitives   : NO
Use Clock Enable                   : Yes
Use Synchronous Set                : Yes
Use Synchronous Reset              : Yes
Pack IO Registers into IOBs        : Auto
Equivalent register Removal        : YES

---- General Options
Optimization Goal                  : Speed
Optimization Effort                : 1
Keep Hierarchy                     : No
Netlist Hierarchy                  : As_Optimized
RTL Output                         : Yes
Global Optimization                : AllClockNets
Read Cores                         : YES
Write Timing Constraints           : NO
Cross Clock Analysis               : NO
Hierarchy Separator                : /
Bus Delimiter                      : <>
Case Specifier                     : Maintain
Slice Utilization Ratio            : 100
BRAM Utilization Ratio             : 100
Verilog 2001                       : YES
Auto BRAM Packing                  : NO
Slice Utilization Ratio Delta      : 5

=========================================================================


=========================================================================
*                          HDL Compilation                              *
=========================================================================
Compiling vhdl file "C:/Temp/Bomberman/hdl/system.vhd" in Library work.
Entity <system> compiled.
Entity <system> (Architecture <STRUCTURE>) compiled.
Compiling vhdl file "C:/Temp/BombermanISE/top.vhd" in Library work.
Entity <top> compiled.
Entity <top> (Architecture <Behavioral>) compiled.

=========================================================================
*                     Design Hierarchy Analysis                         *
=========================================================================
Analyzing hierarchy for entity <top> in library <work> (architecture <Behavioral>).

Analyzing hierarchy for entity <system> in library <work> (architecture <STRUCTURE>).


=========================================================================
*                            HDL Analysis                               *
=========================================================================
Analyzing Entity <top> in library <work> (Architecture <Behavioral>).
Entity <top> analyzed. Unit <top> generated.

Analyzing Entity <system> in library <work> (Architecture <STRUCTURE>).
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'MB_Halted' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Instruction' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Valid_Instr' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_PC' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Reg_Write' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Reg_Addr' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_MSR_Reg' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_PID_Reg' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_New_Reg_Value' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Exception_Taken' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Exception_Kind' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Jump_Taken' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Delay_Slot' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Address' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Access' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Read' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Write' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Write_Value' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Data_Byte_Enable' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_DCache_Req' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_DCache_Hit' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_DCache_Rdy' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_DCache_Read' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_ICache_Req' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_ICache_Hit' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_ICache_Rdy' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_OF_PipeRun' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_EX_PipeRun' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_MEM_PipeRun' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_MB_Halted' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'Trace_Jump_Hit' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL0_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL1_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL2_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL3_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL4_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL5_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL6_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL7_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL8_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL9_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL10_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL11_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL12_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL13_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL14_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_S_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_S_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_M_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_M_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_M_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'FSL15_M_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_IN_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_IN_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_OUT_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_OUT_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_OUT_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'ICACHE_FSL_OUT_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_IN_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_IN_READ' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_OUT_CLK' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_OUT_WRITE' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_OUT_DATA' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1602: Unconnected output port 'DCACHE_FSL_OUT_CONTROL' of component 'microblaze_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_Rst' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'MPLB_Rst' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_dcrAck' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_dcrDBus' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SaddrAck' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SMRdErr' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SMWrErr' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SMBusy' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SrdBTerm' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SrdComp' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SrdDAck' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SrdDBus' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SrdWdAddr' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_Srearbitrate' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_Sssize' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_Swait' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SwrBTerm' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SwrComp' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'PLB_SwrDAck' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 1907: Unconnected output port 'Bus_Error_Det' of component 'mb_plb_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2114: Unconnected output port 'IP2INTC_Irpt' of component 'leds_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2114: Unconnected output port 'GPIO_IO_T' of component 'leds_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2114: Unconnected output port 'GPIO2_IO_O' of component 'leds_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2114: Unconnected output port 'GPIO2_IO_T' of component 'leds_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2167: Unconnected output port 'IP2INTC_Irpt' of component 'led_7segment_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2167: Unconnected output port 'GPIO_IO_T' of component 'led_7segment_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2167: Unconnected output port 'GPIO2_IO_O' of component 'led_7segment_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2167: Unconnected output port 'GPIO2_IO_T' of component 'led_7segment_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2220: Unconnected output port 'IP2INTC_Irpt' of component 'push_buttons_3bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2220: Unconnected output port 'GPIO_IO_O' of component 'push_buttons_3bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2220: Unconnected output port 'GPIO_IO_T' of component 'push_buttons_3bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2220: Unconnected output port 'GPIO2_IO_O' of component 'push_buttons_3bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2220: Unconnected output port 'GPIO2_IO_T' of component 'push_buttons_3bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2273: Unconnected output port 'IP2INTC_Irpt' of component 'switches_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2273: Unconnected output port 'GPIO_IO_O' of component 'switches_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2273: Unconnected output port 'GPIO_IO_T' of component 'switches_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2273: Unconnected output port 'GPIO2_IO_O' of component 'switches_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2273: Unconnected output port 'GPIO2_IO_T' of component 'switches_8bit_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2326: Unconnected output port 'Interrupt' of component 'rs232_port_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH0_Access_Full' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH0_ReadData_Control' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH0_ReadData_Data' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH0_ReadData_Exists' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH1_Access_Full' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH1_ReadData_Control' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH1_ReadData_Data' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH1_ReadData_Exists' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH2_Access_Full' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH2_ReadData_Control' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH2_ReadData_Data' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH2_ReadData_Exists' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH3_Access_Full' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH3_ReadData_Control' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH3_ReadData_Data' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'MCH3_ReadData_Exists' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_RPN' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_CEN' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_QWEN' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_CE' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_ADV_LDN' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_LBON' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_CKEN' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2375: Unconnected output port 'Mem_RNW' of component 'micron_ram_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2469: Unconnected output port 'GenerateOut0' of component 'xps_timer_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2469: Unconnected output port 'GenerateOut1' of component 'xps_timer_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2469: Unconnected output port 'PWM0' of component 'xps_timer_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2469: Unconnected output port 'Interrupt' of component 'xps_timer_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT1' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT2' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT3' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT4' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT5' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT6' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT7' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT8' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT9' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT10' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT11' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT12' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT13' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT14' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKOUT15' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'CLKFBOUT' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2522: Unconnected output port 'PSDONE' of component 'clock_generator_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Interrupt' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'MDM_DBus' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'MDM_errAck' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'MDM_retry' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'MDM_toutSup' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'MDM_xferAck' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_2' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_3' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_4' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_5' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_6' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Clk_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_TDI_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Reg_En_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Capture_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Shift_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Update_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Dbg_Rst_7' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_tdi' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_reset' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_shift' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_update' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_capture' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_sel1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'bscan_drck1' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_S_CLK' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_S_READ' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_M_CLK' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_M_WRITE' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_M_DATA' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'FSL0_M_CONTROL' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_DRCK' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_RESET' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_SEL' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_CAPTURE' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_SHIFT' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_UPDATE' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2551: Unconnected output port 'Ext_JTAG_TDI' of component 'mdm_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetcore_0' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetchip_0' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetsys_0' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetcore_1' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetchip_1' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'RstcPPCresetsys_1' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2704: Unconnected output port 'Peripheral_Reset' of component 'proc_sys_reset_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2728: Unconnected output port 'IP2INTC_Irpt_2' of component 'xps_ps2_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2728: Unconnected output port 'PS2_2_DATA_O' of component 'xps_ps2_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2728: Unconnected output port 'PS2_2_DATA_T' of component 'xps_ps2_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2728: Unconnected output port 'PS2_2_CLK_O' of component 'xps_ps2_0_wrapper'.
WARNING:Xst:753 - "C:/Temp/Bomberman/hdl/system.vhd" line 2728: Unconnected output port 'PS2_2_CLK_T' of component 'xps_ps2_0_wrapper'.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2932: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2940: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2948: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2956: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2964: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2972: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2980: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2988: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 2996: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3004: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3012: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3020: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3028: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3036: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3044: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3052: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3060: Instantiating black box module <IOBUF>.
WARNING:Xst:2211 - "C:/Temp/Bomberman/hdl/system.vhd" line 3068: Instantiating black box module <IOBUF>.
Entity <system> analyzed. Unit <system> generated.


=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Performing bidirectional port resolution...

Synthesizing Unit <system>.
    Related source file is "C:/Temp/Bomberman/hdl/system.vhd".
WARNING:Xst:646 - Signal <pgassign3<0:8>> is assigned but never used. This unconnected signal will be trimmed during the optimization process.
WARNING:Xst:646 - Signal <pgassign2> is assigned but never used. This unconnected signal will be trimmed during the optimization process.
Unit <system> synthesized.


Synthesizing Unit <top>.
    Related source file is "C:/Temp/BombermanISE/top.vhd".
Unit <top> synthesized.


=========================================================================
HDL Synthesis Report

Found no macro
=========================================================================

=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================


=========================================================================
Advanced HDL Synthesis Report

Found no macro
=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================

Optimizing unit <top> ...

Optimizing unit <system> ...

Mapping all equations...
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VS_pin> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_WEN_pin> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_HS_pin> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_RS232_PORT_TX_pin> driven by black box <rs232_port_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_OEN_pin> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<9>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<10>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<11>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<12>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<13>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<14>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<15>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<16>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<17>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<18>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<19>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<20>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<21>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<22>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<23>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<24>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<25>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<26>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<27>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<28>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<29>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<30>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_A_pin<31>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<0>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<1>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<2>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<3>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<4>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<5>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<6>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<7>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<8>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<9>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<10>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LED_7SEGMENT_GPIO_IO_O_pin<11>> driven by black box <led_7segment_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<0>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<1>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<2>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<3>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<4>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<5>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<6>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_LEDs_8Bit_GPIO_IO_O_pin<7>> driven by black box <leds_8bit_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_BEN_pin<0>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <fpga_0_Micron_RAM_Mem_BEN_pin<1>> driven by black box <micron_ram_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<0>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<1>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<2>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<3>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<4>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<5>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<6>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
WARNING:Xst:2036 - Inserting OBUF on port <graph_acc_0_VGA_rgb_pin<7>> driven by black box <graph_acc_0_wrapper>. Possible simulation mismatch.
Building and optimizing final netlist ...
Found area constraint ratio of 100 (+ 5) on block top, actual ratio is 0.

Final Macro Processing ...

=========================================================================
Final Register Report

Found no macro
=========================================================================

=========================================================================
*                           Partition Report                            *
=========================================================================

Partition Implementation Status
-------------------------------

  No Partitions were found in this design.

-------------------------------

=========================================================================
*                            Final Report                               *
=========================================================================
Final Results
RTL Top Level Output File Name     : top.ngr
Top Level Output File Name         : top
Output Format                      : NGC
Optimization Goal                  : Speed
Keep Hierarchy                     : No

Design Statistics
# IOs                              : 90

Cell Usage :
# BELS                             : 1
#      GND                         : 1
# IO Buffers                       : 90
#      IBUF                        : 14
#      IOBUF                       : 18
#      OBUF                        : 58
# Others                           : 21
#      clock_generator_0_wrapper   : 1
#      dlmb_cntlr_wrapper          : 1
#      dlmb_wrapper                : 1
#      graph_acc_0_wrapper         : 1
#      ilmb_cntlr_wrapper          : 1
#      ilmb_wrapper                : 1
#      led_7segment_wrapper        : 1
#      leds_8bit_wrapper           : 1
#      lmb_bram_wrapper            : 1
#      mb_plb_wrapper              : 1
#      mdm_0_wrapper               : 1
#      microblaze_0_wrapper        : 1
#      micron_ram_wrapper          : 1
#      my_timer_0_wrapper          : 1
#      proc_sys_reset_0_wrapper    : 1
#      push_buttons_3bit_wrapper   : 1
#      rs232_port_wrapper          : 1
#      switches_8bit_wrapper       : 1
#      xps_intc_0_wrapper          : 1
#      xps_ps2_0_wrapper           : 1
#      xps_timer_0_wrapper         : 1
=========================================================================

Device utilization summary:
---------------------------

Selected Device : 3s1200efg320-4 

 Number of Slices:                        0  out of   8672     0%  
 Number of IOs:                          90
 Number of bonded IOBs:                  90  out of    250    36%  

---------------------------
Partition Resource Summary:
---------------------------

  No Partitions were found in this design.

---------------------------


=========================================================================
TIMING REPORT

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.
      FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT
      GENERATED AFTER PLACE-and-ROUTE.

Clock Information:
------------------
No clock signals found in this design

Asynchronous Control Signals Information:
----------------------------------------
No asynchronous control signals found in this design

Timing Summary:
---------------
Speed Grade: -4

   Minimum period: No path found
   Minimum input arrival time before clock: No path found
   Maximum output required time after clock: No path found
   Maximum combinational path delay: 3.692ns

Timing Detail:
--------------
All values displayed in nanoseconds (ns)

=========================================================================
Timing constraint: Default path analysis
  Total number of paths / destination ports: 3524 / 3506
-------------------------------------------------------------------------
Delay:               3.692ns (Levels of Logic = 1)
  Source:            Inst_system/xps_ps2_0:PS2_1_CLK_O (PAD)
  Destination:       xps_ps2_0_PS2_1_CLK (PAD)

  Data Path: Inst_system/xps_ps2_0:PS2_1_CLK_O to xps_ps2_0_PS2_1_CLK
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
    xps_ps2_0_wrapper:PS2_1_CLK_O    1   0.000   0.420  Inst_system/xps_ps2_0 (Inst_system/xps_ps2_0_PS2_1_CLK_O)
     IOBUF:I->IO               3.272          Inst_system/iobuf_17 (xps_ps2_0_PS2_1_CLK)
    ----------------------------------------
    Total                      3.692ns (3.272ns logic, 0.420ns route)
                                       (88.6% logic, 11.4% route)

=========================================================================


Total REAL time to Xst completion: 13.00 secs
Total CPU time to Xst completion: 12.67 secs
 
--> 

Total memory usage is 158648 kilobytes

Number of errors   :    0 (   0 filtered)
Number of warnings :  388 (   0 filtered)
Number of infos    :    0 (   0 filtered)

