
# ##############################################################################
# Created by Base System Builder Wizard for Xilinx EDK 12.2 Build EDK_MS2.63c
# Mon Sep 12 15:38:38 2011
# Target Board:  Digilent Nexys 2-1200 Board Rev C
# Family:    spartan3e
# Device:    XC3S1200E
# Package:   FG320
# Speed Grade:  -4
# Processor number: 1
# Processor 1: microblaze_0
# System clock frequency: 50.0
# Debug Interface: On-Chip HW Debug Module
# ##############################################################################
 PARAMETER VERSION = 2.1.0


 PORT fpga_0_LEDs_8Bit_GPIO_IO_O_pin = fpga_0_LEDs_8Bit_GPIO_IO_O_pin, DIR = O, VEC = [0:7]
 PORT fpga_0_LED_7SEGMENT_GPIO_IO_O_pin = fpga_0_LED_7SEGMENT_GPIO_IO_O_pin, DIR = O, VEC = [0:11]
 PORT fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin = fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin, DIR = I, VEC = [0:2]
 PORT fpga_0_Switches_8Bit_GPIO_IO_I_pin = fpga_0_Switches_8Bit_GPIO_IO_I_pin, DIR = I, VEC = [0:7]
 PORT fpga_0_RS232_PORT_RX_pin = fpga_0_RS232_PORT_RX_pin, DIR = I
 PORT fpga_0_RS232_PORT_TX_pin = fpga_0_RS232_PORT_TX_pin, DIR = O
 PORT fpga_0_Micron_RAM_Mem_A_pin = fpga_0_Micron_RAM_Mem_A_pin_vslice_9_31_concat, DIR = O, VEC = [9:31]
 PORT fpga_0_Micron_RAM_Mem_OEN_pin = fpga_0_Micron_RAM_Mem_OEN_pin, DIR = O
 PORT fpga_0_Micron_RAM_Mem_WEN_pin = fpga_0_Micron_RAM_Mem_WEN_pin, DIR = O
 PORT fpga_0_Micron_RAM_Mem_BEN_pin = fpga_0_Micron_RAM_Mem_BEN_pin, DIR = O, VEC = [0:1]
 PORT fpga_0_Micron_RAM_Mem_DQ_pin = fpga_0_Micron_RAM_Mem_DQ_pin, DIR = IO, VEC = [0:15]
 PORT fpga_0_clk_1_sys_clk_pin = dcm_clk_s, DIR = I, SIGIS = CLK, CLK_FREQ = 50000000
 PORT fpga_0_rst_1_sys_rst_pin = sys_rst_s, DIR = I, SIGIS = RST, RST_POLARITY = 1
 PORT xps_ps2_0_PS2_1_DATA = xps_ps2_0_PS2_1_DATA, DIR = IO
 PORT xps_ps2_0_PS2_1_CLK = xps_ps2_0_PS2_1_CLK, DIR = IO
 PORT graph_acc_0_HS_pin = graph_acc_0_HS, DIR = O
 PORT graph_acc_0_VS_pin = graph_acc_0_VS, DIR = O
 PORT graph_acc_0_VGA_rgb_pin = graph_acc_0_VGA_rgb, DIR = O, VEC = [0:7]


BEGIN microblaze
 PARAMETER INSTANCE = microblaze_0
 PARAMETER C_AREA_OPTIMIZED = 1
 PARAMETER C_DEBUG_ENABLED = 1
 PARAMETER HW_VER = 7.30.b
 BUS_INTERFACE DLMB = dlmb
 BUS_INTERFACE ILMB = ilmb
 BUS_INTERFACE DPLB = mb_plb
 BUS_INTERFACE IPLB = mb_plb
 BUS_INTERFACE DEBUG = microblaze_0_mdm_bus
 PORT MB_RESET = mb_reset
 PORT INTERRUPT = microblaze_0_INTERRUPT
END

BEGIN plb_v46
 PARAMETER INSTANCE = mb_plb
 PARAMETER HW_VER = 1.04.a
 PORT PLB_Clk = clk_50_0000MHz
 PORT SYS_Rst = sys_bus_reset
END

BEGIN lmb_v10
 PARAMETER INSTANCE = ilmb
 PARAMETER HW_VER = 1.00.a
 PORT LMB_Clk = clk_50_0000MHz
 PORT SYS_Rst = sys_bus_reset
END

BEGIN lmb_v10
 PARAMETER INSTANCE = dlmb
 PARAMETER HW_VER = 1.00.a
 PORT LMB_Clk = clk_50_0000MHz
 PORT SYS_Rst = sys_bus_reset
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = dlmb_cntlr
 PARAMETER HW_VER = 2.10.b
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x00007fff
 BUS_INTERFACE SLMB = dlmb
 BUS_INTERFACE BRAM_PORT = dlmb_port
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = ilmb_cntlr
 PARAMETER HW_VER = 2.10.b
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x00007fff
 BUS_INTERFACE SLMB = ilmb
 BUS_INTERFACE BRAM_PORT = ilmb_port
END

BEGIN bram_block
 PARAMETER INSTANCE = lmb_bram
 PARAMETER HW_VER = 1.00.a
 BUS_INTERFACE PORTA = ilmb_port
 BUS_INTERFACE PORTB = dlmb_port
END

BEGIN xps_gpio
 PARAMETER INSTANCE = LEDs_8Bit
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_GPIO_WIDTH = 8
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81440000
 PARAMETER C_HIGHADDR = 0x8144ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT GPIO_IO_O = fpga_0_LEDs_8Bit_GPIO_IO_O_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = LED_7SEGMENT
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_GPIO_WIDTH = 12
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81460000
 PARAMETER C_HIGHADDR = 0x8146ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT GPIO_IO_O = fpga_0_LED_7SEGMENT_GPIO_IO_O_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = Push_Buttons_3Bit
 PARAMETER C_ALL_INPUTS = 1
 PARAMETER C_GPIO_WIDTH = 3
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81420000
 PARAMETER C_HIGHADDR = 0x8142ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT GPIO_IO_I = fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = Switches_8Bit
 PARAMETER C_ALL_INPUTS = 1
 PARAMETER C_GPIO_WIDTH = 8
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81400000
 PARAMETER C_HIGHADDR = 0x8140ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT GPIO_IO_I = fpga_0_Switches_8Bit_GPIO_IO_I_pin
END

BEGIN xps_uartlite
 PARAMETER INSTANCE = RS232_PORT
 PARAMETER C_BAUDRATE = 9600
 PARAMETER C_DATA_BITS = 8
 PARAMETER C_USE_PARITY = 0
 PARAMETER C_ODD_PARITY = 0
 PARAMETER HW_VER = 1.01.a
 PARAMETER C_BASEADDR = 0x84000000
 PARAMETER C_HIGHADDR = 0x8400ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT RX = fpga_0_RS232_PORT_RX_pin
 PORT TX = fpga_0_RS232_PORT_TX_pin
END

BEGIN xps_mch_emc
 PARAMETER INSTANCE = Micron_RAM
 PARAMETER C_NUM_BANKS_MEM = 1
 PARAMETER C_NUM_CHANNELS = 0
 PARAMETER C_MEM0_WIDTH = 16
 PARAMETER C_MAX_MEM_WIDTH = 16
 PARAMETER C_INCLUDE_DATAWIDTH_MATCHING_0 = 1
 PARAMETER C_SYNCH_MEM_0 = 0
 PARAMETER C_TCEDV_PS_MEM_0 = 85000
 PARAMETER C_TAVDV_PS_MEM_0 = 85000
 PARAMETER C_THZCE_PS_MEM_0 = 8000
 PARAMETER C_THZOE_PS_MEM_0 = 8000
 PARAMETER C_TWC_PS_MEM_0 = 85000
 PARAMETER C_TWP_PS_MEM_0 = 55000
 PARAMETER C_TLZWE_PS_MEM_0 = 5000
 PARAMETER HW_VER = 3.01.a
 PARAMETER C_MEM0_BASEADDR = 0x82000000
 PARAMETER C_MEM0_HIGHADDR = 0x82ffffff
 BUS_INTERFACE SPLB = mb_plb
 PORT RdClk = clk_50_0000MHz
 PORT Mem_A = 0b000000000 & fpga_0_Micron_RAM_Mem_A_pin_vslice_9_31_concat
 PORT Mem_OEN = fpga_0_Micron_RAM_Mem_OEN_pin
 PORT Mem_WEN = fpga_0_Micron_RAM_Mem_WEN_pin
 PORT Mem_BEN = fpga_0_Micron_RAM_Mem_BEN_pin
 PORT Mem_DQ = fpga_0_Micron_RAM_Mem_DQ_pin
END

BEGIN xps_timer
 PARAMETER INSTANCE = xps_timer_0
 PARAMETER C_COUNT_WIDTH = 32
 PARAMETER C_ONE_TIMER_ONLY = 0
 PARAMETER HW_VER = 1.02.a
 PARAMETER C_BASEADDR = 0x83c00000
 PARAMETER C_HIGHADDR = 0x83c0ffff
 BUS_INTERFACE SPLB = mb_plb
END

BEGIN clock_generator
 PARAMETER INSTANCE = clock_generator_0
 PARAMETER C_CLKIN_FREQ = 50000000
 PARAMETER C_CLKOUT0_FREQ = 50000000
 PARAMETER C_CLKOUT0_PHASE = 0
 PARAMETER C_CLKOUT0_GROUP = NONE
 PARAMETER C_CLKOUT0_BUF = TRUE
 PARAMETER C_EXT_RESET_HIGH = 1
 PARAMETER HW_VER = 4.00.a
 PORT CLKIN = dcm_clk_s
 PORT CLKOUT0 = clk_50_0000MHz
 PORT RST = sys_rst_s
 PORT LOCKED = Dcm_all_locked
END

BEGIN mdm
 PARAMETER INSTANCE = mdm_0
 PARAMETER C_MB_DBG_PORTS = 1
 PARAMETER C_USE_UART = 1
 PARAMETER C_UART_WIDTH = 8
 PARAMETER HW_VER = 1.00.g
 PARAMETER C_BASEADDR = 0x84400000
 PARAMETER C_HIGHADDR = 0x8440ffff
 BUS_INTERFACE SPLB = mb_plb
 BUS_INTERFACE MBDEBUG_0 = microblaze_0_mdm_bus
 PORT Debug_SYS_Rst = Debug_SYS_Rst
END

BEGIN proc_sys_reset
 PARAMETER INSTANCE = proc_sys_reset_0
 PARAMETER C_EXT_RESET_HIGH = 1
 PARAMETER HW_VER = 2.00.a
 PORT Slowest_sync_clk = clk_50_0000MHz
 PORT Ext_Reset_In = sys_rst_s
 PORT MB_Debug_Sys_Rst = Debug_SYS_Rst
 PORT Dcm_locked = Dcm_all_locked
 PORT MB_Reset = mb_reset
 PORT Bus_Struct_Reset = sys_bus_reset
 PORT Peripheral_Reset = sys_periph_reset
END

BEGIN xps_ps2
 PARAMETER INSTANCE = xps_ps2_0
 PARAMETER HW_VER = 1.01.b
 PARAMETER C_BASEADDR = 0x86a00000
 PARAMETER C_HIGHADDR = 0x86a0ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT IP2INTC_Irpt_1 = xps_ps2_0_IP2INTC_Irpt_1
 PORT PS2_1_DATA = xps_ps2_0_PS2_1_DATA
 PORT PS2_1_CLK = xps_ps2_0_PS2_1_CLK
END

BEGIN xps_intc
 PARAMETER INSTANCE = xps_intc_0
 PARAMETER HW_VER = 2.01.a
 PARAMETER C_BASEADDR = 0x81800000
 PARAMETER C_HIGHADDR = 0x8180ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT Intr = xps_ps2_0_IP2INTC_Irpt_1 & my_timer_0_IP2INTC_Irpt
 PORT Irq = microblaze_0_INTERRUPT
END

BEGIN my_timer
 PARAMETER INSTANCE = my_timer_0
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_BASEADDR = 0xc0a00000
 PARAMETER C_HIGHADDR = 0xc0a0ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT IP2INTC_Irpt = my_timer_0_IP2INTC_Irpt
END

BEGIN graph_acc
 PARAMETER INSTANCE = graph_acc_0
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_BASEADDR = 0xc1e00000
 PARAMETER C_HIGHADDR = 0xc1e0ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT HS = graph_acc_0_HS
 PORT VS = graph_acc_0_VS
 PORT VGA_rgb = graph_acc_0_VGA_rgb
END

