#Please do not modify this file by hand
XmpVersion: 12.2
VerMgmt: 12.2
IntStyle: ise
ModuleSearchPath: C:/Temp/Digilent_Nexys_EDK_Board_Support_Files_V_2_1/lib
MHS File: system.mhs
MSS File: system.mss
Architecture: spartan3e
Device: xc3s1200e
Package: fg320
SpeedGrade: -4
UserCmd1: 
UserCmd1Type: 0
UserCmd2: 
UserCmd2Type: 0
GenSimTB: 0
SdkExportBmmBit: 1
SdkExportDir: SDK/SDK_Export
InsertNoPads: 1
WarnForEAArch: 1
HdlLang: vhdl
SimModel: BEHAVIORAL
UcfFile: data/system.ucf
EnableParTimingError: 1
ShowLicenseDialog: 1
Processor: microblaze_0
BootLoop: 0
XmdStub: 0
SwProj: TestApp_Memory_microblaze_0
Processor: microblaze_0
Executable: TestApp_Memory_microblaze_0/executable.elf
Source: TestApp_Memory_microblaze_0/src/TestApp_Memory.c
DefaultInit: EXECUTABLE
InitBram: 0
Active: 1
CompilerOptLevel: 2
GlobPtrOpt: 0
DebugSym: 1
ProfileFlag: 0
ProgStart: 
StackSize: 
HeapSize: 
LinkerScript: TestApp_Memory_microblaze_0/src/TestApp_Memory_LinkScr.ld
ProgCCFlags: 
CompileInXps: 1
NonXpsApp: 0
SwProj: TestApp_Peripheral_microblaze_0
Processor: microblaze_0
Executable: TestApp_Peripheral_microblaze_0/executable.elf
Source: TestApp_Peripheral_microblaze_0/src/TestApp_Peripheral.c
Source: TestApp_Peripheral_microblaze_0/src/xgpio_tapp_example.c
Source: TestApp_Peripheral_microblaze_0/src/xtmrctr_selftest_example.c
Source: TestApp_Peripheral_microblaze_0/src/xuartlite_selftest_example.c
Header: TestApp_Peripheral_microblaze_0/src/gpio_header.h
Header: TestApp_Peripheral_microblaze_0/src/tmrctr_header.h
Header: TestApp_Peripheral_microblaze_0/src/uartlite_header.h
Header: microblaze_0/include/graph_acc.h
DefaultInit: EXECUTABLE
InitBram: 0
Active: 1
CompilerOptLevel: 2
GlobPtrOpt: 0
DebugSym: 1
ProfileFlag: 0
ProgStart: 
StackSize: 
HeapSize: 
LinkerScript: 
ProgCCFlags: 
CompileInXps: 1
NonXpsApp: 0
SwProj: Testproj
Processor: microblaze_0
Executable: Testproj/executable.elf
Source: TestApp_Peripheral_microblaze_0/src/xuartlite_selftest_example.c
Source: TestApp_Peripheral_microblaze_0/src/TestApp_Peripheral.c
Source: TestApp_Peripheral_microblaze_0/src/xgpio_tapp_example.c
Source: TestApp_Peripheral_microblaze_0/src/xtmrctr_selftest_example.c
Source: drivers/my_timer_selftest.c
Source: drivers/my_timer.c
Header: TestApp_Peripheral_microblaze_0/src/uartlite_header.h
Header: TestApp_Peripheral_microblaze_0/src/gpio_header.h
Header: TestApp_Peripheral_microblaze_0/src/tmrctr_header.h
Header: drivers/graph_acc_v1_00_a/src/graph_acc.h
Header: drivers/my_timer.h
Header: scancodes.h
DefaultInit: EXECUTABLE
InitBram: 1
Active: 1
CompilerOptLevel: 4
GlobPtrOpt: 0
DebugSym: 1
ProfileFlag: 0
ProgStart: 
StackSize: 
HeapSize: 300
LinkerScript: 
ProgCCFlags: 
CompileInXps: 1
NonXpsApp: 0
SwProj: Intc_test
Processor: microblaze_0
Executable: Intc_test/executable.elf
Source: example.c
Header: TestApp_Peripheral_microblaze_0/src/uartlite_header.h
Header: scancodes.h
DefaultInit: executable
InitBram: 0
Active: 1
CompilerOptLevel: 2
GlobPtrOpt: 0
DebugSym: 1
ProfileFlag: 0
ProgStart: 
StackSize: 
HeapSize: 
LinkerScript: 
ProgCCFlags: 
CompileInXps: 1
NonXpsApp: 0
SwProj: Timer_itnr_test
Processor: microblaze_0
Executable: Timer_itnr_test/executable.elf
Source: drivers/my_timer_selftest.c
Source: drivers/my_timer.c
Source: timer_intr_test.c
Header: drivers/my_timer.h
DefaultInit: executable
InitBram: 0
Active: 1
CompilerOptLevel: 2
GlobPtrOpt: 0
DebugSym: 1
ProfileFlag: 0
ProgStart: 
StackSize: 
HeapSize: 
LinkerScript: 
ProgCCFlags: 
CompileInXps: 1
NonXpsApp: 0
