<?xml version="1.0" encoding="UTF-8" standalone="yes" ?>
<document OS="nt" product="ISE" version="12.2">

  <!--The data in this file is primarily intended for consumption by Xilinx tools.
    The structure and the elements are likely to change over the next few releases.
    This means code written to parse this file will need to be revisited each subsequent release.-->

  <application stringID="par" timeStamp="Tue Oct 04 11:38:08 2011">
    <section stringID="User_Env">
      <table stringID="User_EnvVar">
        <column stringID="variable"/>
        <column stringID="value"/>
        <row stringID="row" value="0">
          <item stringID="variable" value="Path"/>
          <item stringID="value" value="C:\Xilinx\12.2\ISE_DS\ISE\\lib\nt;C:\Xilinx\12.2\ISE_DS\ISE\\bin\nt;C:\Xilinx\12.2\ISE_DS\PlanAhead\bin;C:\Xilinx\12.2\ISE_DS\ISE\bin\nt;C:\Xilinx\12.2\ISE_DS\ISE\lib\nt;C:\Xilinx\12.2\ISE_DS\EDK\bin\nt;C:\Xilinx\12.2\ISE_DS\EDK\lib\nt;C:\Xilinx\12.2\ISE_DS\common\bin\nt;C:\Xilinx\12.2\ISE_DS\common\lib\nt;C:\Program Files\Autodesk\Alias2010\bin;C:\WINDOWS\system32;C:\WINDOWS;C:\WINDOWS\system32\Wbem;C:\Program Files\Common Files\Adobe\AGL;C:\Program Files\QuickTime\QTSystem\C:\Program Files\proeWildfire 5.0\bin;C:\WINDOWS\system32\WindowsPowerShell\v1.0;C:\Program Files\Rayfront\platform\win32\bin;C:\Program Files\Matlab\R2010a\bin\;C:\Program Files\Microsoft Visual Studio 10.0\Vc\bin;C:\Program Files\Microsoft SDKs\Windows\v7.0A\bin;C:\Program Files\Microsoft Visual Studio 10.0\Common7\IDE;C:\Program Files\QuickTime\QTSystem\"/>
        </row>
        <row stringID="row" value="1">
          <item stringID="variable" value="PATHEXT"/>
          <item stringID="value" value=".COM;.EXE;.BAT;.CMD;.VBS;.VBE;.JS;.JSE;.WSF;.WSH;.PSC1"/>
        </row>
        <row stringID="row" value="2">
          <item stringID="variable" value="XILINX"/>
          <item stringID="value" value="C:\Xilinx\12.2\ISE_DS\ISE\"/>
        </row>
        <row stringID="row" value="3">
          <item stringID="variable" value="XILINXD_LICENSE_FILE"/>
          <item stringID="value" value="2100@vm05.cs.lth.se"/>
        </row>
        <row stringID="row" value="4">
          <item stringID="variable" value="XILINX_DSP"/>
          <item stringID="value" value="C:\Xilinx\12.2\ISE_DS\ISE"/>
        </row>
        <row stringID="row" value="5">
          <item stringID="variable" value="XILINX_EDK"/>
          <item stringID="value" value="C:\Xilinx\12.2\ISE_DS\EDK"/>
        </row>
        <row stringID="row" value="6">
          <item stringID="variable" value="XILINX_PLANAHEAD"/>
          <item stringID="value" value="C:\Xilinx\12.2\ISE_DS\PlanAhead"/>
        </row>
      </table>
      <item stringID="User_EnvOs" value="OS Information">
        <item stringID="User_EnvOsname" value="Microsoft Windows XP Professional"/>
        <item stringID="User_EnvOsrelease" value="Service Pack 3  (build 2600)"/>
      </item>
      <item stringID="User_EnvHost" value="neptunus-6"/>
      <table stringID="User_EnvCpu">
        <column stringID="arch"/>
        <column stringID="speed"/>
        <row stringID="row" value="0">
          <item stringID="arch" value="AMD Athlon(tm) 64 X2 Dual Core Processor 4000+"/>
          <item stringID="speed" value="2094 MHz"/>
        </row>
      </table>
    </section>
    <task stringID="PAR_OPTION_SUMMARY">
      <section stringID="PAR_OPTION_SUMMARY">
        <item DEFAULT="1" label="-t" stringID="PAR_COSTTABLE_ENTRY" value="1"/>
        <item DEFAULT="" label="-intstyle" stringID="PAR_INTSTYLE" value="ise"/>
        <item DEFAULT="std" label="-ol" stringID="PAR_OVERALL_EFFORTLEVEL" value="high"/>
        <item DEFAULT="false" label="-w" stringID="PAR_OVERWRITE_OUTPUT" value="true"/>
      </section>
    </task>
    <task stringID="PAR_DEVICE_UTILIZATION">
      <section stringID="PAR_DESIGN_SUMMARY"></section>
    </task>
    <task stringID="PAR_PAR">
      <section stringID="PAR_DESIGN_SUMMARY">
        <item stringID="PAR_REAL_TIME_COMPLETION_ROUTER" value="12 mins 1 secs "/>
        <item stringID="PAR_CPU_TIME_COMPLETION_ROUTER" value="11 mins 54 secs "/>
        <item dataType="int" stringID="PAR_UNROUTES" value="0"/>
        <item dataType="float" stringID="PAR_TIMING_SCORE" value="0.000000"/>
        <item stringID="PAR_REAL_TIME_COMPLETION_PAR" value="12 mins 9 secs "/>
        <item stringID="PAR_CPU_TIME_COMPLETION_PAR" value="12 mins 2 secs "/>
      </section>
    </task>
    <task stringID="PAR_par">
      <section stringID="PAR_DLY_CLK_REPORT"/>
      <section stringID="PAR_CLOCK_REPORT">
        <table stringID="PAR_CLOCK_TABLE">
          <column label="Clock Net" stringID="CLOCK_NET"/>
          <column label="Routed" stringID="ROUTED"/>
          <column label="Resource" stringID="RESOURCE"/>
          <column label="Locked" stringID="LOCKED"/>
          <column label="Fanout" stringID="FANOUT"/>
          <column label="Net Skew(ns)" stringID="NET_SKEW"/>
          <column label="Max Delay(ns)" stringID="MAX_DELAY"/>
          <row stringID="row" value="1">
            <item label="Clock Net" stringID="CLOCK_NET" value="Inst_system/clk_50_0000MHz"/>
            <item label="Routed" stringID="ROUTED" value="ROUTED"/>
            <item label="Resource" stringID="RESOURCE" value="BUFGMUX_X1Y10"/>
            <item label="Locked" stringID="LOCKED" value="No"/>
            <item dataType="float" label="Fanout" stringID="FANOUT" value="2775.000000"/>
            <item dataType="float" label="Net Skew(ns)" stringID="NET_SKEW" value="0.212000"/>
            <item dataType="float" label="Max Delay(ns)" stringID="MAX_DELAY" value="0.381000"/>
          </row>
          <row stringID="row" value="2">
            <item label="Clock Net" stringID="CLOCK_NET" value="Inst_system/mdm_0/Dbg_Clk_1"/>
            <item label="Routed" stringID="ROUTED" value="ROUTED"/>
            <item label="Resource" stringID="RESOURCE" value="BUFGMUX_X1Y0"/>
            <item label="Locked" stringID="LOCKED" value="No"/>
            <item dataType="float" label="Fanout" stringID="FANOUT" value="109.000000"/>
            <item dataType="float" label="Net Skew(ns)" stringID="NET_SKEW" value="0.138000"/>
            <item dataType="float" label="Max Delay(ns)" stringID="MAX_DELAY" value="0.317000"/>
          </row>
          <row stringID="row" value="3">
            <item label="Clock Net" stringID="CLOCK_NET" value="Inst_system/mdm_0/Dbg_Update_1"/>
            <item label="Routed" stringID="ROUTED" value="ROUTED"/>
            <item label="Resource" stringID="RESOURCE" value="Local"/>
            <item dataType="float" label="Fanout" stringID="FANOUT" value="24.000000"/>
            <item dataType="float" label="Net Skew(ns)" stringID="NET_SKEW" value="1.882000"/>
            <item dataType="float" label="Max Delay(ns)" stringID="MAX_DELAY" value="3.794000"/>
          </row>
          <row stringID="row" value="4">
            <item label="Clock Net" stringID="CLOCK_NET" value="fpga_0_clk_1_sys_clk_pin_IBUF"/>
            <item label="Routed" stringID="ROUTED" value="ROUTED"/>
            <item label="Resource" stringID="RESOURCE" value="Local"/>
            <item dataType="float" label="Fanout" stringID="FANOUT" value="4.000000"/>
            <item dataType="float" label="Net Skew(ns)" stringID="NET_SKEW" value="0.539000"/>
            <item dataType="float" label="Max Delay(ns)" stringID="MAX_DELAY" value="1.993000"/>
          </row>
        </table>
      </section>
      <section stringID="PAR_PAD_PIN_REPORT">
        <table stringID="PAR_PINOUT_BY_PIN_NUMBER">
          <column label="Pin&#xA;Number" sort="smart" stringID="Pin_Number"/>
          <column label="Signal&#xA;Name" stringID="Signal_Name"/>
          <column label="Pin&#xA;Usage" stringID="Pin_Usage"/>
          <column label="Pin&#xA;Name" sort="smart" stringID="Pin_Name"/>
          <column stringID="Direction"/>
          <column label="IO&#xA;Standard" sort="smart" stringID="IO_Standard"/>
          <column label="IO Bank&#xA;Number" stringID="IO_Bank_Number"/>
          <column label="Drive&#xA;(mA)" stringID="Drive"/>
          <column label="Slew&#xA;Rate" stringID="Slew_Rate"/>
          <column label="Termination" stringID="Termination"/>
          <column label="IOB&#xA;Delay" stringID="IOB_Delay"/>
          <column label="Voltage" stringID="Voltage"/>
          <column label="Constraint" stringID="Constraint"/>
          <column label="IO&#xA;Register" stringID="IO_Register"/>
          <column label="Signal&#xA;Integrity" stringID="Signal_Integrity"/>
          <row stringID="row" value="1">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A1"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="2">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A2"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="TDI"/>
          </row>
          <row stringID="row" value="3">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="4">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="5">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L22P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="6">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="7">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="8">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="9">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A9"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_0"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="10">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12N_0/GCLK7"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="11">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="12">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="13">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="14">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="15">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L02N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="16">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="17">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="TCK"/>
          </row>
          <row stringID="row" value="18">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="A18"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="19">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B1"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="PROG_B"/>
          </row>
          <row stringID="row" value="20">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B2"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="21">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L25N_0/HSWAP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="22">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="23">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L22N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="24">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="25">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="26">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B8"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_clk_1_sys_clk_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L13P_0/GCLK8"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="27">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L13N_0/GCLK9"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="28">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12P_0/GCLK6"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="29">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="30">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="31">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05N_0/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="32">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="33">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L02P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="34">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="35">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="36">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="B18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_rst_1_sys_rst_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="37">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;13>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="38">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;14>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="39">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L25P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="40">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="41">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="42">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C6"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_0"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="43">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="44">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L16P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="45">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14P_0/GCLK10"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="46">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C10"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="47">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="48">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L07P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="49">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C13"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_0"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="50">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03N_0/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="51">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="52">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C16"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="TDO"/>
          </row>
          <row stringID="row" value="53">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;4>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24N_1/LDC2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="54">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="C18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24P_1/LDC1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="55">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;10>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L02P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="56">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;12>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L02N_3/VREF_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="57">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="58">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="59">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23N_0/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="60">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="61">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18N_0/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="62">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L16N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="63">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14N_0/GCLK11"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="64">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11P_0/GCLK4"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="65">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="66">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L07N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="67">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="68">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="69">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D15"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="TMS"/>
          </row>
          <row stringID="row" value="70">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D16"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;8>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23N_1/LDC0"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="71">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;9>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23P_1/HDC"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="72">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="D18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP/VREF_1"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="73">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;17>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="74">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;15>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="75">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04N_3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="76">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="77">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E5"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="78">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="79">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19N_0/VREF_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="80">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="81">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="82">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11N_0/GCLK5"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="83">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="84">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="85">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="86">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E14"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="87">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="88">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E16"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;3>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22N_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="89">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E17"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="90">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="E18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="91">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;23>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="92">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;18>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="93">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F3"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_3"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="94">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="95">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="96">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F6"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="97">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="98">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="99">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="100">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L10P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="101">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="102">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06P_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="103">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F13"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="104">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="105">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F15"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21P_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="106">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F16"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_1"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="107">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;3>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19N_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="108">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="F18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;10>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19P_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="109">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G1"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="110">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G2"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="111">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;22>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="112">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;19>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06N_3/VREF_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="113">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;20>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="114">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;21>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="115">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="116">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_0"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="117">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="118">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L10N_0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
          </row>
          <row stringID="row" value="119">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_0"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="0"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="120">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="121">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="122">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G14"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;7>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20P_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="123">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="124">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="125">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="126">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="G18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;7>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="127">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;28>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="128">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;27>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="129">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;25>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="130">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;29>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="131">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08N_3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="132">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;24>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="133">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_3"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="134">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="135">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H9"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="136">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H10"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="137">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="138">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_1"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="139">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H13"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="140">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H14"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;5>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17P_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="141">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="142">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="143">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16N_1/A0"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="144">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="H18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;6>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP/VREF_1"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="145">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;31>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12P_3/LHCLK2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="146">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;30>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12N_3/LHCLK3/IRDY2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="147">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J3"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="148">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11N_3/LHCLK1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="149">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;26>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11P_3/LHCLK0"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="150">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP/VREF_3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="151">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="152">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="153">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="154">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15P_1/A2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="155">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15N_1/A1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="156">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J14"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;7>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14N_1/A3/RHCLK7"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="157">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J15"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;6>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14P_1/A4/RHCLK6"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="158">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13N_1/A5/RHCLK5"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="159">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;6>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13P_1/A6/RHCLK4/IRDY1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="160">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="J18"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_1"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="161">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K1"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_3"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="162">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K2"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="163">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;11>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13P_3/LHCLK4/TRDY2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="164">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_BEN_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13N_3/LHCLK5"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="PULLDOWN"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="165">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_BEN_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14N_3/LHCLK7"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="PULLDOWN"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="166">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;9>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L14P_3/LHCLK6"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="167">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="168">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="169">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="170">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11N_1/A9/RHCLK1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="171">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L11P_1/A10/RHCLK0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="172">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K14"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;4>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12N_1/A7/RHCLK3/TRDY1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="173">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K15"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;5>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12P_1/A8/RHCLK2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="174">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K16"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="175">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;4>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="176">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="K18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;5>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="177">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;15>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="178">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;3>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="179">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;7>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="180">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;14>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="181">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;6>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17N_3/VREF_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="182">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;13>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L17P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="183">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_3"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="184">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="185">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L9"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="186">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L10"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="187">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="188">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_1"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="189">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L13"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="190">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L14"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;3>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="191">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09N_1/A11"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="192">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09P_1/A12"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="193">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L17"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10N_1/VREF_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="194">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="L18"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LED_7SEGMENT_GPIO_IO_O_pin&lt;11>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10P_1"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="195">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M1"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="196">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M2"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="197">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;5>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="198">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;12>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="199">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_A_pin&lt;16>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="200">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;4>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="201">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="202">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M8"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_2"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="203">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12N_2/D6/GCLK13"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="204">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16P_2/M0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="205">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M11"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_2"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="206">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="207">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05N_1/VREF_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="208">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="209">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="210">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="211">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="212">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="M18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="213">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N1"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="214">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N2"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="215">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N3"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_3"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="216">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="217">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;11>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="218">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N6"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="219">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N7"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_WEN_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07P_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="220">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N8"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;3>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09N_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="221">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L12P_2/D7/GCLK12"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="222">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L16N_2/DIN/D0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="223">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="224">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="225">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N13"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="226">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="227">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="228">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N16"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_1"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="229">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="230">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="N18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L08P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="231">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;10>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="232">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;9>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="233">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22P_3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="234">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22N_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="235">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P5"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="236">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;5>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05N_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="237">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L07N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="238">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P8"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;4>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L09P_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="239">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P9"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_RS232_PORT_TX_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="240">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15N_2/D1/GCLK3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="241">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P11"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="xps_ps2_0_PS2_1_DATA"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L18P_2"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="242">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L21N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="243">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22P_2/A23"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="244">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P14"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCINT"/>
            <item label="Voltage" stringID="Voltage" value="1.2"/>
          </row>
          <row stringID="row" value="245">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="246">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P16"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_LEDs_8Bit_GPIO_IO_O_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="12"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="247">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P17"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="248">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="P18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06N_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="249">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R1"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="250">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;8>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="251">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L23P_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="252">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP/VREF_3"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="253">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="254">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L05P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="255">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L08N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="256">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R8"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;2>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10P_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="257">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R9"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO/D5"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="258">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L15P_2/D2/GCLK2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="259">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="260">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R12"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="xps_ps2_0_PS2_1_CLK"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20N_2"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="261">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L22N_2/A22"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="262">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24N_2/A20"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="263">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03P_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="264">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03N_1/VREF_1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="265">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R17"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Switches_8Bit_GPIO_IO_I_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="266">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="R18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L02P_1/A14"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="267">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T1"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_DQ_pin&lt;0>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24N_3"/>
            <item stringID="Direction" value="BIDIR"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="YES"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="268">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T2"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_Micron_RAM_Mem_OEN_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24P_3"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="PULLUP"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="269">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01N_2/INIT_B"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="270">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_HS_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03N_2/MOSI/CSI_B"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="271">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L04N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="272">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T6"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_2"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="273">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L08P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="274">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T8"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;1>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L10N_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="275">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T9"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="276">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L14N_2/M2/GCLK1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="277">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L17P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="278">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L20P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="279">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T13"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_2"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="280">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L24P_2/A21"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="281">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO/VREF_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="282">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L26P_2/VS0/A17"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="283">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T17"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01N_1/A15"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="284">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="T18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L02N_1/A13"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="285">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U1"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="3"/>
          </row>
          <row stringID="row" value="286">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U2"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="287">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U3"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VS_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01P_2/CSO_B"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="288">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U4"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;7>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L03P_2/DOUT/BUSY"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="289">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U5"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="graph_acc_0_VGA_rgb_pin&lt;6>"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO/VREF_2"/>
            <item stringID="Direction" value="OUTPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Drive&#xA;(mA)" stringID="Drive" value="2"/>
            <item label="Slew&#xA;Rate" stringID="Slew_Rate" value="SLOW"/>
            <item label="Termination" stringID="Termination" value="NONE**"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="290">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U6"/>
            <item label="Signal&#xA;Name" stringID="Signal_Name" value="fpga_0_RS232_PORT_RX_pin"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="INPUT"/>
            <item label="IO&#xA;Standard" sort="smart" stringID="IO_Standard" value="LVCMOS33"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Termination" stringID="Termination" value="PULLUP"/>
            <item label="IOB&#xA;Delay" stringID="IOB_Delay" value="NONE"/>
            <item label="Constraint" stringID="Constraint" value="LOCATED"/>
            <item label="IO&#xA;Register" stringID="IO_Register" value="NO"/>
            <item label="Signal&#xA;Integrity" stringID="Signal_Integrity" value="NONE"/>
          </row>
          <row stringID="row" value="291">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U7"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="292">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L11P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="293">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13P_2/D4/GCLK14"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="294">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U10"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L14P_2/RDWR_B/GCLK0"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="295">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L17N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="296">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U12"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCAUX"/>
            <item label="Voltage" stringID="Voltage" value="2.5"/>
          </row>
          <row stringID="row" value="297">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="298">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L23N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="299">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L25N_2/VS1/A18"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="300">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L26N_2/CCLK"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="301">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="302">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="U18"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L01P_1/A16"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="1"/>
          </row>
          <row stringID="row" value="303">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V1"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
          <row stringID="row" value="304">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V2"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="305">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V3"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L02N_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="306">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V4"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L02P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="307">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V5"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="308">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V6"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L06N_2/VREF_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="309">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V7"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="310">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V8"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFSI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L11N_2/VREF_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="311">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V9"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L13N_2/D3/GCLK15"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="312">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V10"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="VCCO_2"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
            <item label="Voltage" stringID="Voltage" value="3.30"/>
          </row>
          <row stringID="row" value="313">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V11"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IOB"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO/M1"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="314">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V12"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="315">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V13"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFS"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L19N_2/VREF_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="316">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V14"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFMI"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP_L23P_2"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="317">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V15"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="DIFFM"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IO_L25P_2/VS2/A19"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="318">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V16"/>
            <item label="Pin&#xA;Usage" stringID="Pin_Usage" value="IBUF"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="IP"/>
            <item stringID="Direction" value="UNUSED"/>
            <item label="IO Bank&#xA;Number" stringID="IO_Bank_Number" value="2"/>
          </row>
          <row stringID="row" value="319">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V17"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="DONE"/>
          </row>
          <row stringID="row" value="320">
            <item label="Pin&#xA;Number" sort="smart" stringID="Pin_Number" value="V18"/>
            <item label="Pin&#xA;Name" sort="smart" stringID="Pin_Name" value="GND"/>
          </row>
        </table>
        <table stringID="PAR_PSEUDO_LOGIC">
          <column label="Signal&#xA;Name" stringID="Signal_Name"/>
          <column stringID="Type"/>
          <column stringID="Site"/>
        </table>
      </section>
      <section stringID="PAR_UNROUTES_REPORT">
        <item dataType="int" stringID="PAR_UNROUTED_NETS" value="0"/>
        <item dataType="int" stringID="PAR_TOTAL_SOURCELESS_NETS" value="0"/>
        <item dataType="int" stringID="PAR_TOTAL_LOADLESS_NETS" value="0"/>
      </section>
    </task>
  </application>

</document>
