// BMM LOC annotation file.
//
// Release 12.2 - Data2MEM M.63c, build 1.7 Jun 25, 2010
// Copyright (c) 1995-2011 Xilinx, Inc.  All rights reserved.


///////////////////////////////////////////////////////////////////////////////
//
// Processor 'microblaze_0', ID 100, memory map.
//
///////////////////////////////////////////////////////////////////////////////

ADDRESS_MAP microblaze_0 MICROBLAZE 100


    ///////////////////////////////////////////////////////////////////////////////
    //
    // Processor 'microblaze_0' address space 'lmb_bram_combined' 0x00000000:0x00007FFF (32 KBytes).
    //
    ///////////////////////////////////////////////////////////////////////////////

    ADDRESS_SPACE lmb_bram_combined RAMB16 [0x00000000:0x00007FFF]
        BUS_BLOCK
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_0 [31:30] PLACED = X0Y10;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_1 [29:28] PLACED = X1Y8;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_2 [27:26] PLACED = X1Y7;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_3 [25:24] PLACED = X1Y9;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_4 [23:22] PLACED = X0Y7;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_5 [21:20] PLACED = X0Y4;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_6 [19:18] PLACED = X0Y3;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_7 [17:16] PLACED = X0Y9;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_8 [15:14] PLACED = X0Y11;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_9 [13:12] PLACED = X0Y8;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_10 [11:10] PLACED = X0Y5;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_11 [9:8] PLACED = X0Y13;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_12 [7:6] PLACED = X0Y12;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_13 [5:4] PLACED = X0Y6;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_14 [3:2] PLACED = X0Y1;
            Inst_system/lmb_bram/lmb_bram/ramb16_s2_s2_15 [1:0] PLACED = X0Y2;
        END_BUS_BLOCK;
    END_ADDRESS_SPACE;

END_ADDRESS_MAP;

