##############################################################
#
# Xilinx Core Generator version 12.2
# Date: Tue Oct 04 08:29:11 2011
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = VHDL
SET device = xc3s1200e
SET devicefamily = spartan3e
SET flowvendor = Foundation_ISE
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = fg320
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -4
SET verilogsim = true
SET vhdlsim = true
# END Project Options
# BEGIN Select
SELECT Block_Memory_Generator family Xilinx,_Inc. 4.2
# END Select
# BEGIN Parameters
CSET additional_inputs_for_power_estimation=false
CSET algorithm=Minimum_Area
CSET assume_synchronous_clk=false
CSET byte_size=9
CSET coe_file=H:\matlab\all.coe
CSET collision_warnings=ALL
CSET component_name=BRAM_imgs
CSET disable_collision_warnings=false
CSET disable_out_of_range_warnings=false
CSET ecc=false
CSET ecctype=No_ECC
CSET enable_a=Always_Enabled
CSET enable_b=Always_Enabled
CSET error_injection_type=Single_Bit_Error_Injection
CSET fill_remaining_memory_locations=false
CSET load_init_file=true
CSET memory_type=Single_Port_ROM
CSET operating_mode_a=WRITE_FIRST
CSET operating_mode_b=WRITE_FIRST
CSET output_reset_value_a=0
CSET output_reset_value_b=0
CSET pipeline_stages=0
CSET port_a_clock=100
CSET port_a_enable_rate=100
CSET port_a_write_rate=0
CSET port_b_clock=0
CSET port_b_enable_rate=0
CSET port_b_write_rate=0
CSET primitive=8kx2
CSET read_width_a=8
CSET read_width_b=8
CSET register_porta_input_of_softecc=false
CSET register_porta_output_of_memory_core=false
CSET register_porta_output_of_memory_primitives=false
CSET register_portb_output_of_memory_core=false
CSET register_portb_output_of_memory_primitives=false
CSET register_portb_output_of_softecc=false
CSET remaining_memory_locations=0
CSET reset_memory_latch_a=false
CSET reset_memory_latch_b=false
CSET reset_priority_a=CE
CSET reset_priority_b=CE
CSET reset_type=SYNC
CSET softecc=false
CSET use_byte_write_enable=false
CSET use_error_injection_pins=false
CSET use_regcea_pin=false
CSET use_regceb_pin=false
CSET use_rsta_pin=false
CSET use_rstb_pin=false
CSET write_depth_a=6144
CSET write_width_a=8
CSET write_width_b=8
# END Parameters
GENERATE
# CRC: 6c38c0c5
