
-- VHDL Instantiation Created from source file system.vhd -- 15:38:03 10/03/2011
--
-- Notes: 
-- 1) This instantiation template has been automatically generated using types
-- std_logic and std_logic_vector for the ports of the instantiated module
-- 2) To use this template to instantiate this entity, cut-and-paste and then edit

	COMPONENT system
	PORT(
		fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin : IN std_logic_vector(0 to 2);
		fpga_0_Switches_8Bit_GPIO_IO_I_pin : IN std_logic_vector(0 to 7);
		fpga_0_RS232_PORT_RX_pin : IN std_logic;
		fpga_0_clk_1_sys_clk_pin : IN std_logic;
		fpga_0_rst_1_sys_rst_pin : IN std_logic;    
		fpga_0_Micron_RAM_Mem_DQ_pin : INOUT std_logic_vector(0 to 15);
		xps_ps2_0_PS2_1_DATA : INOUT std_logic;
		xps_ps2_0_PS2_1_CLK : INOUT std_logic;      
		fpga_0_LEDs_8Bit_GPIO_IO_O_pin : OUT std_logic_vector(0 to 7);
		fpga_0_LED_7SEGMENT_GPIO_IO_O_pin : OUT std_logic_vector(0 to 11);
		fpga_0_RS232_PORT_TX_pin : OUT std_logic;
		fpga_0_Micron_RAM_Mem_A_pin : OUT std_logic_vector(9 to 31);
		fpga_0_Micron_RAM_Mem_OEN_pin : OUT std_logic;
		fpga_0_Micron_RAM_Mem_WEN_pin : OUT std_logic;
		fpga_0_Micron_RAM_Mem_BEN_pin : OUT std_logic_vector(0 to 1);
		graph_acc_0_HS_pin : OUT std_logic;
		graph_acc_0_VS_pin : OUT std_logic;
		graph_acc_0_VGA_rgb_pin : OUT std_logic_vector(0 to 7)
		);
	END COMPONENT;

attribute box_type : string;
attribute box_type of system : component is "user_black_box";


	Inst_system: system PORT MAP(
		fpga_0_LEDs_8Bit_GPIO_IO_O_pin => ,
		fpga_0_LED_7SEGMENT_GPIO_IO_O_pin => ,
		fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin => ,
		fpga_0_Switches_8Bit_GPIO_IO_I_pin => ,
		fpga_0_RS232_PORT_RX_pin => ,
		fpga_0_RS232_PORT_TX_pin => ,
		fpga_0_Micron_RAM_Mem_A_pin => ,
		fpga_0_Micron_RAM_Mem_OEN_pin => ,
		fpga_0_Micron_RAM_Mem_WEN_pin => ,
		fpga_0_Micron_RAM_Mem_BEN_pin => ,
		fpga_0_Micron_RAM_Mem_DQ_pin => ,
		fpga_0_clk_1_sys_clk_pin => ,
		fpga_0_rst_1_sys_rst_pin => ,
		xps_ps2_0_PS2_1_DATA => ,
		xps_ps2_0_PS2_1_CLK => ,
		graph_acc_0_HS_pin => ,
		graph_acc_0_VS_pin => ,
		graph_acc_0_VGA_rgb_pin => 
	);



