<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="UtilitiesC" num="159" delta="old" >Message file &quot;<arg fmt="%s" index="1">usenglish/ip.msg</arg>&quot; wasn&apos;t found.
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">4</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">4</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_input_block.vhd</arg>&quot; line <arg fmt="%d" index="2">88</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_input_block.vhd</arg>&quot; line <arg fmt="%d" index="2">88</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">780</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%s" index="1">$Id: get_init_bmg_v4_2.c,v 1.1.2.1 2010/04/01 12:39:27 muruga Exp $</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:\Temp\BombermanISE\ipcore_dir\.\tmp\_cg\BRAM_imgs.mif</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:\Temp\BombermanISE\ipcore_dir\.\tmp\_cg\BRAM_imgs.mif</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%s" index="1">$Id: get_init_bmg_v4_2.c,v 1.1.2.1 2010/04/01 12:39:27 muruga Exp $</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:\Temp\BombermanISE\ipcore_dir\.\tmp\_cg\BRAM_imgs.mif</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%s" index="1">$Id: get_init_bmg_v4_2.c,v 1.1.2.1 2010/04/01 12:39:27 muruga Exp $</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:\Temp\BombermanISE\ipcore_dir\.\tmp\_cg\BRAM_imgs.mif</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">4</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">4</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">4</arg>x<arg fmt="%d" index="5">4096</arg> 	u:<arg fmt="%d" index="6">4</arg>
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_input_block.vhd</arg>&quot; line <arg fmt="%d" index="2">691</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_input_block.vhd</arg>&quot; line <arg fmt="%d" index="2">707</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1539</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1552</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="752" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected input port &apos;<arg fmt="%s" index="3">ADDR_IN</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos; is tied to default value.
</msg>

<msg type="warning" file="Xst" num="752" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected input port &apos;<arg fmt="%s" index="3">SBITERRIN</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos; is tied to default value.
</msg>

<msg type="warning" file="Xst" num="752" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected input port &apos;<arg fmt="%s" index="3">DBITERRIN</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos; is tied to default value.
</msg>

<msg type="warning" file="Xst" num="753" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected output port &apos;<arg fmt="%s" index="3">SBITERR</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos;.
</msg>

<msg type="warning" file="Xst" num="753" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected output port &apos;<arg fmt="%s" index="3">DBITERR</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos;.
</msg>

<msg type="warning" file="Xst" num="753" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%d" index="2">1599</arg>: Unconnected output port &apos;<arg fmt="%s" index="3">RDADDRECC</arg>&apos; of component &apos;<arg fmt="%s" index="4">blk_mem_gen_mux</arg>&apos;.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">976</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addra_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">977</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addrb_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">976</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addra_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">977</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addrb_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">976</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addra_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="2096" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_prim_width.vhd</arg>&quot; line <arg fmt="%d" index="2">977</arg>: Use of null array slice on signal &lt;<arg fmt="%s" index="3">addrb_pad</arg>&gt; is not supported.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">470</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">472</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">872</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="info" file="Xst" num="2679" delta="old" >Register &lt;<arg fmt="%s" index="1">rdaddrecc_lat</arg>&gt; in unit &lt;<arg fmt="%s" index="2">blk_mem_gen_mux.1</arg>&gt; has a constant value of <arg fmt="%s" index="3">0000000000000</arg> during circuit operation. The register is replaced by logic.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">470</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">472</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="warning" file="Xst" num="795" delta="old" >&quot;<arg fmt="%s" index="1">C:/Temp/BombermanISE/ipcore_dir/./tmp/_cg/_bbx/blk_mem_gen_v4_2/blk_mem_gen_mux.vhd</arg>&quot; line <arg fmt="%d" index="2">872</arg>: Size of operands are different : result is &lt;false&gt;.
</msg>

<msg type="info" file="Xst" num="2679" delta="old" >Register &lt;<arg fmt="%s" index="1">rdaddrecc_lat</arg>&gt; in unit &lt;<arg fmt="%s" index="2">blk_mem_gen_mux.2</arg>&gt; has a constant value of <arg fmt="%s" index="3">0000000000000</arg> during circuit operation. The register is replaced by logic.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ENA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">INJECTSBITERR_I</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RSTA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RSTB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WEA&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WEB&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DINA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">INJECTDBITERR_I</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RDADDRECC_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DOUTB_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">SBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">ERROR_INTERNAL</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">DECODER_DOUTB</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">DECODER_DOUTA</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_LAT_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ADDR_IN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_REGCE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_REG_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MUX_REGCE&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MUX_RST&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">SBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_lat</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_LAT_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ADDR_IN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_REGCE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MEM_REG_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MUX_REGCE&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">MUX_RST&lt;0&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">SBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_lat</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b&lt;31:4&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a&lt;31:4&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b&lt;31:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a&lt;31:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_a9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_b&lt;35:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a&lt;35:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_din_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b&lt;3:1&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a&lt;3:1&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b&lt;31:8&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a&lt;31:8&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b&lt;3:1&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a&lt;3:1&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b&lt;31:8&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a&lt;31:8&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_a9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_b&lt;35:9&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a&lt;35:9&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_din_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_b</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_doutp_a</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_b&lt;31:4&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dout_a&lt;31:4&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0000000000000000000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_b</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a4</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_dinp_a</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_b&lt;31:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a32</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_din_a&lt;31:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_a9</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_b&lt;35:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_dout_a&lt;35:4&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">full_din_a72</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">doutb_pad&lt;8&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">douta_pad&lt;8&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="1305" delta="old" >Output &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0000000000000</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">sbiterr_sdp</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">sbiterr_array</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">00000000</arg>.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">rst_enb</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">rst_ena</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_reg</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_out</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_lat</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">rdaddrecc_last</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_sbiterr1</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_sbiterr0</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_sbiterr</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_dbiterr1</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_dbiterr0</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ram_dbiterr</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">enb_array&lt;3&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">ena_array&lt;3&gt;</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">doutb_array&lt;31:24&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">00000000</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">douta_array&lt;31:24&gt;</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">00000000</arg>.
</msg>

<msg type="warning" file="Xst" num="646" delta="old" >Signal &lt;<arg fmt="%s" index="1">dbiterr_sdp</arg>&gt; is assigned but never used. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">dbiterr_array</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">00000000</arg>.
</msg>

<msg type="warning" file="Xst" num="1780" delta="old" >Signal &lt;<arg fmt="%s" index="1">addrb_in</arg>&gt; is never used or assigned. This unconnected signal will be trimmed during the optimization process.
</msg>

<msg type="info" file="Xst" num="2261" delta="old" >The FF/Latch &lt;<arg fmt="%s" index="1">has_mux_b.B/sel_pipe_1</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">blk_mem_gen_generic_cstr</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">FF/Latch</arg>, which will be removed : <arg fmt="%s" index="4">&lt;has_mux_b.B/sel_pipe_0&gt; </arg>
</msg>

<msg type="warning" file="Xst" num="1293" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">has_mux_b.B/sel_pipe_1</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">blk_mem_gen_generic_cstr</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="info" file="Xst" num="2169" delta="old" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

