[Inputs]
fpga_0_RS232_PORT_RX_pin
fpga_0_clk_1_sys_clk_pin
fpga_0_rst_1_sys_rst_pin
=fpga_0_Push_Buttons_3Bit_GPIO_IO_I_pin[0:2]=
=fpga_0_Switches_8Bit_GPIO_IO_I_pin[0:7]=
[Outputs]
fpga_0_RS232_PORT_TX_pin
fpga_0_Micron_RAM_Mem_OEN_pin
fpga_0_Micron_RAM_Mem_WEN_pin
graph_acc_0_HS_pin
graph_acc_0_VS_pin
=fpga_0_LEDs_8Bit_GPIO_IO_O_pin[0:7]=
=fpga_0_LED_7SEGMENT_GPIO_IO_O_pin[0:11]=
=fpga_0_Micron_RAM_Mem_A_pin[9:31]=
=fpga_0_Micron_RAM_Mem_BEN_pin[0:1]=
=graph_acc_0_VGA_rgb_pin[0:7]=
[BiDir]
xps_ps2_0_PS2_1_DATA
xps_ps2_0_PS2_1_CLK
=fpga_0_Micron_RAM_Mem_DQ_pin[0:15]=
