Par Statistics
Total Non-vccgnd Signals= 8870
Total Non-vccgnd Design Pins= 35793
Total Non-vccgnd Conns= 35793
Total Non-vccgnd Timing Constrained Conns= 33605
Phase 1 CPU= 9.5 sec
Phase 2 CPU= 10.5 sec
Phase 3 CPU= 18.7 sec
Phase 4 CPU= 19.6 sec
Phase 5 CPU= 35.3 sec
Phase 6 CPU= 35.3 sec
Phase 7 CPU= 35.3 sec
Phase 8 CPU= 35.3 sec
Phase 9 CPU= 35.3 sec
Phase 10 CPU= 37.1 sec
AvgWirelenPerPin Fanout 1= 3.0
AvgWirelenPerPin Fanout 2= 2.5
AvgWirelenPerPin Fanout 3= 3.0
AvgWirelenPerPin Fanout 4= 2.8
AvgWirelenPerPin Fanout 10= 3.6
AvgWirelenPerPin Fanout 50= 4.4
AvgWirelenPerPin Fanout 100= 7.7
AvgWirelenPerPin Fanout 500= 7.4
AvgWirelenPerPin Fanout 5000= 6.9
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 22.0769