#
# pin constraints
#
NET DIP_Switches_8Bits_TRI_I[0] LOC = "T10"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[1] LOC = "T9"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[2] LOC = "V9"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[3] LOC = "M8"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[4] LOC = "N8"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[5] LOC = "U8"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[6] LOC = "V8"  |  IOSTANDARD = "LVCMOS33";
NET DIP_Switches_8Bits_TRI_I[7] LOC = "T5"  |  IOSTANDARD = "LVCMOS33";
NET GCLK LOC = "V10"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[0] LOC = "U16"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[1] LOC = "V16"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[2] LOC = "U15"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[3] LOC = "V15"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[4] LOC = "M11"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[5] LOC = "N11"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[6] LOC = "R11"  |  IOSTANDARD = "LVCMOS33";
NET LEDs_8Bits_TRI_O[7] LOC = "T11"  |  IOSTANDARD = "LVCMOS33";
NET Push_Buttons_4Bits_TRI_I[0] LOC = "A8"  |  IOSTANDARD = "LVCMOS33";
NET Push_Buttons_4Bits_TRI_I[1] LOC = "C4"  |  IOSTANDARD = "LVCMOS33";
NET Push_Buttons_4Bits_TRI_I[2] LOC = "C9"  |  IOSTANDARD = "LVCMOS33";
NET Push_Buttons_4Bits_TRI_I[3] LOC = "D9"  |  IOSTANDARD = "LVCMOS33";
NET RESET LOC = "B8"  |  IOSTANDARD = "LVCMOS33"  |  TIG;
NET RS232_Uart_1_sin LOC = "N17"  |  IOSTANDARD = "LVCMOS33";
NET RS232_Uart_1_sout LOC = "N18"  |  IOSTANDARD = "LVCMOS33";

NET mem_to_vga_0_hs_pin  		LOC = "N6" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_vs_pin  		LOC = "P7" |  IOSTANDARD = "LVCMOS33";

NET mem_to_vga_0_rgb_pin[0]    LOC ="U7" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_rgb_pin[1]    LOC ="V7" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_rgb_pin[2]    LOC ="N7" |  IOSTANDARD = "LVCMOS33";

NET mem_to_vga_0_rgb_pin[3]    LOC ="P8" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_rgb_pin[4]    LOC ="T6" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_rgb_pin[5]    LOC ="V6" |  IOSTANDARD = "LVCMOS33";

NET mem_to_vga_0_rgb_pin[6]   LOC ="R7" |  IOSTANDARD = "LVCMOS33";
NET mem_to_vga_0_rgb_pin[7]   LOC ="T7" |  IOSTANDARD = "LVCMOS33";
#
# additional constraints
#

NET "GCLK" TNM_NET = sys_clk_pin;
TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 100000 kHz;

