xfft_v8_0_vinfo

    CHANGE LOG for Xilinx LogiCORE Fast Fourier Transform 8.0

    Release Date:  June 19, 2013
    --------------------------------------------------------------------------------

    Table of Contents

    1.   INTRODUCTION
    2.   DEVICE SUPPORT
    3.   NEW FEATURE HISTORY
    4.   RESOLVED ISSUES
    5.   KNOWN ISSUES & LIMITATIONS
    6.   TECHNICAL SUPPORT & FEEDBACK
    7.   CORE RELEASE HISTORY
    8.   LEGAL DISCLAIMER

    --------------------------------------------------------------------------------

    1. INTRODUCTION

      This file contains the change log for all released versions of the Xilinx
      LogiCORE IP Fast Fourier Transform.

      For the latest core updates, see the product page at:

        www.xilinx.com/products/ipcenter/FFT.htm

      For installation instructions for this release, please go to:

        www.xilinx.com/ipcenter/coregen/ip_update_install_instructions.htm

      For system requirements:

        www.xilinx.com/ipcenter/coregen/ip_update_system_requirements.htm

    2. DEVICE SUPPORT

      2.1. ISE

        The following device families are supported by the core for this release:

        All Series 7 devices
        All Virtex-6 devices
        All Spartan-6 devices

    3. NEW FEATURE HISTORY

      3.1 ISE

      v8.0
        - Ongoing new device support.
        - AXI4-Stream Interfaces replace old pinout
        - C model available in CORE Generator in 14.1

    4. RESOLVED ISSUES

      4.1 ISE

      v8.0
        1. C model LSB mismatch for odd point sizes, streaming architecture
          - CR546238
          - CR576743
          - CR576806

        2. Tooltip for ARESETN did not indicate active low.
          - CR572366

    5. KNOWN ISSUES & LIMITATIONS

      The following are known issues for this core at time of release:

      5.1 ISE
        1. The core will drop data sent within 2 cycles of the disassertion
           of ARESETN. The workaround is to ensure no transfers are
           attempted for 2 clock cycles following the release of ARESETN.
           - CR 591111.

        2. The bit-accurate C model and Matlab MEX function for the FFT core
           can return incorrect results when configured to perform a Block
           Floating-Point FFT using the Pipelined, Streaming I/O architecture.
          - CR 639407
          - AR 53087

      For a comprehensive listing of Known Issues for this core, please see the IP
      Release Notes Guide,

        www.xilinx.com/support/documentation/user_guides/xtp025.pdf

    6. TECHNICAL SUPPORT & FEEDBACK

      To obtain technical support, create a WebCase at www.xilinx.com/support.
      Questions are routed to a team with expertise using this product.
      Please feel free to leave feedback on this IP under the "Leave Feedback"
      menu item in Vivado/PlanAhead.

      Xilinx provides technical support for use of this product when used
      according to the guidelines described in the core documentation, and
      cannot guarantee timing, functionality, or support of this product for
      designs that do not follow specified guidelines.

    7. CORE RELEASE HISTORY

    Date        By            Version      Description
    ================================================================================
    06/19/2012  Xilinx, Inc.  8.0         ISE 14.6 support
    03/20/2012  Xilinx, Inc.  8.0         ISE 14.5 support.
    12/18/2012  Xilinx, Inc.  8.0         ISE 14.4 and Vivado 2012.4 support
    10/16/2012  Xilinx, Inc.  8.0         ISE 14.3 and Vivado 2012.3 support
    07/25/2012  Xilinx, Inc.  8.0         ISE 14.2 and Vivado 2012.2 support
    04/24/2012  Xilinx, Inc.  8.0         ISE 14.1 support and Vivado 2012.1 support,
                                          C model in CORE Generator
    01/11/2012  Xilinx, Inc.  8.0         ISE 13.4 support
    10/19/2011  Xilinx, Inc.  8.0         ISE 13.3 support
    06/22/2011  Xilinx, Inc.  8.0         ISE 13.2 support, Artix-7 support
    03/01/2011  Xilinx, Inc.  8.0         ISE 13.1 support, Virtex-7 and Kintex-7 support
    09/21/2010  Xilinx, Inc.  8.0         ISE 12.3 support. AXI4-Streaming.
    04/19/2010  Xilinx, Inc.  7.1         ISE 12.1 support. Bugfixes.
    12/02/2009  Xilinx, Inc.  7.0         ISE 11.4 support, Spartan-6L support.
    09/16/2009  Xilinx, Inc.  7.0         ISE 11.3 support, Virtex-6L support.
    06/24/2009  Xilinx, Inc.  7.0         ISE 11.2 support, Virtex-6/Spartan-6 support.
    09/19/2008  Xilinx, Inc.  6.0         ISE 10.1 support. Features added. Bugfixes.
    10/10/2007  Xilinx, Inc.  5.0         ISE 9.2i support. Features added. Bugfixes.
    ================================================================================

    8. LEGAL DISCLAIMER

      (c) Copyright 2000 - 2013 Xilinx, Inc. All rights reserved.

      This file contains confidential and proprietary information
      of Xilinx, Inc. and is protected under U.S. and
      international copyright and other intellectual property
      laws.

      DISCLAIMER
      This disclaimer is not a license and does not grant any
      rights to the materials distributed herewith. Except as
      otherwise provided in a valid license issued to you by
      Xilinx, and to the maximum extent permitted by applicable
      law: (1) THESE MATERIALS ARE MADE AVAILABLE "AS IS" AND
      WITH ALL FAULTS, AND XILINX HEREBY DISCLAIMS ALL WARRANTIES
      AND CONDITIONS, EXPRESS, IMPLIED, OR STATUTORY, INCLUDING
      BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY, NON-
      INFRINGEMENT, OR FITNESS FOR ANY PARTICULAR PURPOSE; and
      (2) Xilinx shall not be liable (whether in contract or tort,
      including negligence, or under any other theory of
      liability) for any loss or damage of any kind or nature
      related to, arising under or in connection with these
      materials, including for any direct, or any indirect,
      special, incidental, or consequential loss or damage
      (including loss of data, profits, goodwill, or any type of
      loss or damage suffered as a result of any action brought
      by a third party) even if such damage or loss was
      reasonably foreseeable or Xilinx had been advised of the
      possibility of the same.

      CRITICAL APPLICATIONS
      Xilinx products are not designed or intended to be fail-
      safe, or for use in any application requiring fail-safe
      performance, such as life-support or safety devices or
      systems, Class III medical devices, nuclear facilities,
      applications related to the deployment of airbags, or any
      other applications that could lead to death, personal
      injury, or severe property or environmental damage
      (individually and collectively, "Critical
      Applications"). Customer assumes the sole risk and
      liability of any use of Xilinx products in Critical
      Applications, subject only to applicable laws and
      regulations governing limitations on product liability.

      THIS COPYRIGHT NOTICE AND DISCLAIMER MUST BE RETAINED AS
      PART OF THIS FILE AT ALL TIMES.