<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="Xst" num="37" delta="old" >Detected unknown constraint/property &quot;<arg fmt="%s" index="1">sigis</arg>&quot;. This constraint/property is not supported by the current software release and will be ignored.
</msg>

<msg type="warning" file="Xst" num="37" delta="old" >Detected unknown constraint/property &quot;<arg fmt="%s" index="1">sigis</arg>&quot;. This constraint/property is not supported by the current software release and will be ignored.
</msg>

<msg type="warning" file="Xst" num="37" delta="old" >Detected unknown constraint/property &quot;<arg fmt="%s" index="1">sigis</arg>&quot;. This constraint/property is not supported by the current software release and will be ignored.
</msg>

<msg type="warning" file="Xst" num="37" delta="old" >Detected unknown constraint/property &quot;<arg fmt="%s" index="1">sigis</arg>&quot;. This constraint/property is not supported by the current software release and will be ignored.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">FSL_S_Clk</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">FSL_S_Control</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd</arg>&quot; line <arg fmt="%s" index="2">163</arg>: Output port &lt;<arg fmt="%s" index="3">blank</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">vga</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd</arg>&quot; line <arg fmt="%s" index="2">163</arg>: Output port &lt;<arg fmt="%s" index="3">new_frame</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">vga</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">addr1&lt;31:7&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">addr2&lt;31:9&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_8</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_7</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_0</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_2</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_1</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_6</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_5</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_4</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_3</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_13</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_9</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_10</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_11</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_12</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_14</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_15</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_16</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_17</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_18</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_19</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_20</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_21</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_22</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_23</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_24</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_25</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_26</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_27</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_28</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_29</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_30</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_31</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_32</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_33</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_34</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_35</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_36</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_37</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_38</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_39</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_40</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_41</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_42</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_43</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_44</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_45</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_46</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_47</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_48</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_49</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_50</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_51</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_52</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_53</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_54</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_55</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_56</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_57</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_58</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_59</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_60</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_61</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_62</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_63</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_64</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_65</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_66</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_67</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_68</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_69</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_70</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_71</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_72</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_73</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_74</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_75</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_76</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_77</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_78</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_79</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_80</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_81</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_82</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_83</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_84</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_85</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_86</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_87</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_88</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_89</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_90</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_91</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_92</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_93</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_94</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_95</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_96</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_97</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_98</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_99</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_100</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_101</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_102</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_103</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_104</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_105</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_106</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_107</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_108</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_109</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_110</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_111</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_112</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_113</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_114</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_115</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_116</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_117</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_118</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_119</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_120</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_121</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_122</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_123</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_124</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_125</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_126</arg>&gt;, simulation mismatch.
</msg>

<msg type="warning" file="Xst" num="3035" delta="old" >Index value(s) does not match array range for signal &lt;<arg fmt="%s" index="1">ram_127</arg>&gt;, simulation mismatch.
</msg>

<msg type="info" file="Xst" num="1767" delta="old" >HDL ADVISOR - Resource sharing has identified that some arithmetic operations in this design can share the same physical resources for reduced device utilization. For improved clock frequency you may try to disable resource sharing.
</msg>

<msg type="warning" file="Xst" num="1293" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">offset_0</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_1</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_2</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_3</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_4</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_5</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_6</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_7</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_8</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_127</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_126</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_125</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_124</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_123</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_122</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_121</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_120</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_119</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_118</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_117</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_116</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_115</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_114</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_113</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_112</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_111</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_110</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_109</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_108</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_107</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_106</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_105</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_104</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_103</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_102</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_101</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_100</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_99</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_97</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_98</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_96</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_95</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_94</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_93</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_92</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_91</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_90</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_89</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_88</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_87</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_86</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_85</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_84</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_83</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_82</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_81</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_80</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_79</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_78</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_77</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_76</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_75</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_74</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_73</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_72</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_71</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_70</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_69</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_68</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_67</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_66</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_64</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_65</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_63</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_62</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_61</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_60</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_59</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_58</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_57</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_56</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_55</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_54</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_53</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_52</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_51</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_50</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_49</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_48</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_47</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_46</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_45</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_44</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_43</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_42</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_41</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_40</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_39</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_38</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_37</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_36</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_35</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_34</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_33</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_31</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_32</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_30</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_29</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_28</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_27</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_26</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_25</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_24</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_23</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_22</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_21</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_20</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_19</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_18</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_17</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_16</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_15</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_14</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_12</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_11</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_10</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_9</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_13</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_3</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_4</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_5</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_6</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_1</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_2</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_0</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3230" delta="old" >The RAM description &lt;<arg fmt="%s" index="1">ram/Mram_ram_7</arg>&gt; will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
</msg>

<msg type="info" file="Xst" num="3225" delta="old" >The RAM &lt;<arg fmt="%s" index="1">ram/Mram_ram_8</arg>&gt; will be implemented as BLOCK RAM
</msg>

<msg type="warning" file="Xst" num="1293" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">offset_0</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_1</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_2</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_3</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_4</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_5</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_6</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_7</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">offset_8</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1293" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">fsl_count_0</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">fsl_count_1</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">fsl_count_2</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">fsl_count_7</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">mem_to_vga</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="1293" delta="new" >FF/Latch &lt;<arg fmt="%s" index="1">ram_offset_0</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="1896" delta="old" >Due to other FF/Latch trimming, FF/Latch &lt;<arg fmt="%s" index="1">ram_offset_1</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="2677" delta="old" >Node &lt;<arg fmt="%s" index="1">vga/blank</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">mem_to_vga</arg>&gt;.
</msg>

<msg type="warning" file="Xst" num="1293" delta="old" >FF/Latch &lt;<arg fmt="%s" index="1">vga/hcounter_10</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">mem_to_vga</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

</messages>

