Par Statistics
Total Non-vccgnd Signals= 2714
Total Non-vccgnd Design Pins= 7842
Total Non-vccgnd Conns= 7842
Total Non-vccgnd Timing Constrained Conns= 7781
Phase 1 CPU= 5.1 sec
Phase 2 CPU= 5.6 sec
Phase 3 CPU= 16.2 sec
Phase 4 CPU= 17.1 sec
Phase 5 CPU= 22.4 sec
Phase 6 CPU= 22.4 sec
Phase 7 CPU= 22.4 sec
Phase 8 CPU= 22.4 sec
Phase 9 CPU= 22.5 sec
Phase 10 CPU= 23.2 sec
AvgWirelenPerPin Fanout 1= 4.0
AvgWirelenPerPin Fanout 2= 6.0
AvgWirelenPerPin Fanout 3= 6.0
AvgWirelenPerPin Fanout 4= 5.8
AvgWirelenPerPin Fanout 10= 3.6
AvgWirelenPerPin Fanout 50= 3.8
AvgWirelenPerPin Fanout 100= 6.2
AvgWirelenPerPin Fanout 500= 2.4
AvgWirelenPerPin Fanout 5000= 2.1
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 5.5199