##############################################################################
## Filename:          D:\workspace\xilinx\xps\test4\pcores/fsl_to_axi_v1_00_a/data/fsl_to_axi_v2_1_0.mpd
## Description:       Microprocessor Peripheral Description
## Date:              Tue Oct 08 10:25:10 2013 (by Create and Import Peripheral Wizard)
##############################################################################

BEGIN fsl_to_axi

## Peripheral Options
OPTION IPTYPE = PERIPHERAL
OPTION IMP_NETLIST = TRUE
OPTION HDL = VHDL
## Bus Interfaces
BUS_INTERFACE BUS=SFSL, BUS_STD=FSL, BUS_TYPE=SLAVE
BUS_INTERFACE BUS=MFSL, BUS_STD=FSL, BUS_TYPE=MASTER

## Peripheral ports
PORT FSL_Clk = "", DIR=I, SIGIS=Clk, BUS=MFSL:SFSL
PORT FSL_Rst = LMB_Rst, DIR=I, BUS=MFSL:SFSL
PORT FSL_S_Clk = FSL_S_Clk, DIR=I, SIGIS=Clk, BUS=SFSL
PORT FSL_S_Read = FSL_S_Read, DIR=O, BUS=SFSL
PORT FSL_S_Data = FSL_S_Data, DIR=I, VEC=[0:31], BUS=SFSL
PORT FSL_S_Control = FSL_S_Control, DIR=I, BUS=SFSL
PORT FSL_S_Exists = FSL_S_Exists, DIR=I, BUS=SFSL
PORT FSL_M_Clk = FSL_M_Clk, DIR=I, SIGIS=Clk, BUS=MFSL
PORT FSL_M_Write = FSL_M_Write, DIR=O, BUS=MFSL
PORT FSL_M_Data = FSL_M_Data, DIR=O, VEC=[0:31], BUS=MFSL
PORT FSL_M_Control = FSL_M_Control, DIR=O, BUS=MFSL
PORT FSL_M_Full = FSL_M_Full, DIR=I, BUS=MFSL

END