<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="UtilitiesC" num="159" delta="new" >Message file &quot;<arg fmt="%s" index="1">usenglish/ip.msg</arg>&quot; wasn&apos;t found.
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">2048</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">3</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">6144</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">4</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">8192</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">5</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">10240</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">6</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">12288</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">7</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">14336</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">1</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">2048</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">2</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">4096</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">3</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">6144</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">4</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">8192</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">5</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">10240</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">6</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">12288</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">7</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">14336</arg>) 	: <arg fmt="%d" index="4">8</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_input_block.vhd" Line 691: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_input_block.vhd" Line 707: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="746" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 978: Range is empty (null range)
</msg>

<msg type="warning" file="HDLCompiler" num="220" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 978: Assignment ignored
</msg>

<msg type="warning" file="HDLCompiler" num="746" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 979: Range is empty (null range)
</msg>

<msg type="warning" file="HDLCompiler" num="220" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 979: Assignment ignored
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_wrapper_s6.vhd" Line 454: Net &lt;<arg fmt="%s" index="1">pad_addr_b14[13]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_wrapper_s6.vhd" Line 463: Net &lt;<arg fmt="%s" index="1">pad_din_b32[31]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_wrapper_s6.vhd" Line 466: Net &lt;<arg fmt="%s" index="1">pad_dinp_b4[3]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_wrapper_s6.vhd" Line 492: Net &lt;<arg fmt="%s" index="1">doutb_i[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 430: Net &lt;<arg fmt="%s" index="1">dina_pad[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_prim_width.vhd" Line 434: Net &lt;<arg fmt="%s" index="1">dinb_pad[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd" Line 1546: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd" Line 1559: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_mux.vhd" Line 459: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_mux.vhd" Line 470: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_mux.vhd" Line 472: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_mux.vhd" Line 872: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd" Line 447: Net &lt;<arg fmt="%s" index="1">sbiterr_array[15]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="new" >"D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd" Line 448: Net &lt;<arg fmt="%s" index="1">dbiterr_array[15]</arg>&gt; does not have a driver.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">doutb</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">rdaddrecc</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bresp</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rdata</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rresp</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rdaddrecc</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">sbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">dbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_awready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_wready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bvalid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_arready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rlast</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rvalid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_sbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\bram.vhd</arg>&quot; line <arg fmt="%s" index="2">151</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_dbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWADDR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWLEN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWSIZE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWBURST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_WDATA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_WSTRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARADDR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARLEN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARSIZE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARBURST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AClk</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_ARESETN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_WLAST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_WVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_BREADY</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_RREADY</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">S_AXI_INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">S_AXI_BID</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_v7_3_xst</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_BRESP</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">S_AXI_RID</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_v7_3_xst</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RDATA</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RRESP</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_AWREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_WREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_BVALID</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_ARREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RLAST</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RVALID</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">S_AXI_DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RSTA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RSTB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">INJECTDBITERR_I</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">INJECTSBITERR_I</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[0].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[0].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[1].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[1].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[2].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[2].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[3].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[3].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[4].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[4].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[5].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[5].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[6].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[6].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[7].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1342</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[7].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1606</arg>: Output port &lt;<arg fmt="%s" index="3">RDADDRECC</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_a.A</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1606</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_a.A</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1606</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_a.A</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1750</arg>: Output port &lt;<arg fmt="%s" index="3">RDADDRECC</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_b.B</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1750</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_b.B</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="new" >&quot;<arg fmt="%s" index="1">D:\workspace\xilinx\ise\bram_test\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v7_3\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1750</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">has_mux_b.B</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">sbiterr_array</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_generic_cstr</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dbiterr_array</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_generic_cstr</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_1</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_1</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_1</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_1</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_1</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_2</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_2</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_2</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_2</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_2</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_3</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_3</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_3</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_3</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_3</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_4</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_4</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_4</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_4</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_4</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_5</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_5</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_5</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_5</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_5</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_6</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_6</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_6</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_6</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_6</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_7</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_7</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_7</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_7</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_7</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_8</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width_8</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_8</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_8</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="new" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_8</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MUX_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MUX_REGCE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">ADDR_IN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">SBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DBITERRIN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MEM_LAT_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MEM_REG_RST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">MEM_REGCE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">WE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DOUTB_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">RDADDRECC_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">SBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">DBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="new" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="info" file="Xst" num="2261" delta="new" >The FF/Latch &lt;<arg fmt="%s" index="1">has_mux_b.B/sel_pipe_3</arg>&gt; in Unit &lt;<arg fmt="%s" index="2">blk_mem_gen_generic_cstr</arg>&gt; is equivalent to the following <arg fmt="%s" index="3">3 FFs/Latches</arg>, which will be removed : <arg fmt="%s" index="4">&lt;has_mux_b.B/sel_pipe_2&gt; &lt;has_mux_b.B/sel_pipe_1&gt; &lt;has_mux_b.B/sel_pipe_0&gt; </arg>
</msg>

<msg type="warning" file="Xst" num="1293" delta="new" >FF/Latch &lt;<arg fmt="%s" index="1">has_mux_b.B/sel_pipe_3</arg>&gt; has a constant value of <arg fmt="%d" index="2">0</arg> in block &lt;<arg fmt="%s" index="3">blk_mem_gen_generic_cstr</arg>&gt;. This FF/Latch will be trimmed during the optimization process.
</msg>

<msg type="warning" file="Xst" num="2973" delta="new" >All outputs of instance &lt;<arg fmt="%s" index="1">bindec_b.bindec_inst_b</arg>&gt; of block &lt;<arg fmt="%s" index="2">bindec</arg>&gt; are unconnected in block &lt;<arg fmt="%s" index="3">blk_mem_gen_generic_cstr</arg>&gt;. Underlying logic will be removed.
</msg>

<msg type="warning" file="Xst" num="2677" delta="new" >Node &lt;<arg fmt="%s" index="1">has_mux_a.A/sel_pipe_0</arg>&gt; of sequential type is unconnected in block &lt;<arg fmt="%s" index="2">blk_mem_gen_generic_cstr</arg>&gt;.
</msg>

<msg type="info" file="Xst" num="2169" delta="new" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

