Release 14.2 - xst P.28xd (nt64)
Copyright (c) 1995-2012 Xilinx, Inc.  All rights reserved.
--> Parameter TMPDIR set to xst/projnav.tmp


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.08 secs
 
--> Parameter xsthdpdir set to xst


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.08 secs
 
--> Reading design: mem_to_vga.prj

TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Parsing
  3) HDL Elaboration
  4) HDL Synthesis
       4.1) HDL Synthesis Report
  5) Advanced HDL Synthesis
       5.1) Advanced HDL Synthesis Report
  6) Low Level Synthesis
  7) Partition Report
  8) Design Summary
       8.1) Primitive and Black Box Usage
       8.2) Device utilization summary
       8.3) Partition Resource Summary
       8.4) Timing Report
            8.4.1) Clock Information
            8.4.2) Asynchronous Control Signals Information
            8.4.3) Timing Summary
            8.4.4) Timing Details
            8.4.5) Cross Clock Domains Report


=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input File Name                    : "mem_to_vga.prj"
Ignore Synthesis Constraint File   : NO

---- Target Parameters
Output File Name                   : "mem_to_vga"
Output Format                      : NGC
Target Device                      : xc6slx16-2-csg324

---- Source Options
Top Module Name                    : mem_to_vga
Automatic FSM Extraction           : YES
FSM Encoding Algorithm             : Auto
Safe Implementation                : No
FSM Style                          : LUT
RAM Extraction                     : Yes
RAM Style                          : Auto
ROM Extraction                     : Yes
Shift Register Extraction          : YES
ROM Style                          : Auto
Resource Sharing                   : YES
Asynchronous To Synchronous        : NO
Shift Register Minimum Size        : 2
Use DSP Block                      : Auto
Automatic Register Balancing       : No

---- Target Options
LUT Combining                      : Auto
Reduce Control Sets                : Auto
Add IO Buffers                     : YES
Global Maximum Fanout              : 100000
Add Generic Clock Buffer(BUFG)     : 16
Register Duplication               : YES
Optimize Instantiated Primitives   : NO
Use Clock Enable                   : Auto
Use Synchronous Set                : Auto
Use Synchronous Reset              : Auto
Pack IO Registers into IOBs        : Auto
Equivalent register Removal        : YES

---- General Options
Optimization Goal                  : Speed
Optimization Effort                : 1
Power Reduction                    : NO
Keep Hierarchy                     : No
Netlist Hierarchy                  : As_Optimized
RTL Output                         : Yes
Global Optimization                : AllClockNets
Read Cores                         : YES
Write Timing Constraints           : NO
Cross Clock Analysis               : NO
Hierarchy Separator                : /
Bus Delimiter                      : <>
Case Specifier                     : Maintain
Slice Utilization Ratio            : 100
BRAM Utilization Ratio             : 100
DSP48 Utilization Ratio            : 100
Auto BRAM Packing                  : NO
Slice Utilization Ratio Delta      : 5

=========================================================================


=========================================================================
*                          HDL Parsing                                  *
=========================================================================
Parsing VHDL file "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\devl\projnav\vga_controller_640_60.vhd" into library work
Parsing entity <vga_controller_640_60>.
Parsing architecture <Behavioral> of entity <vga_controller_640_60>.
Parsing VHDL file "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\devl\projnav\block_ram.vhd" into library work
Parsing entity <block_ram>.
Parsing architecture <Behavioral> of entity <block_ram>.
Parsing VHDL file "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd" into library mem_to_vga_v1_00_a
Parsing entity <mem_to_vga>.
Parsing architecture <EXAMPLE> of entity <mem_to_vga>.

=========================================================================
*                            HDL Elaboration                            *
=========================================================================

Elaborating entity <mem_to_vga> (architecture <EXAMPLE>) from library <mem_to_vga_v1_00_a>.

Elaborating entity <vga_controller_640_60> (architecture <Behavioral>) from library <work>.

Elaborating entity <block_ram> (architecture <Behavioral>) from library <work>.

=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Synthesizing Unit <mem_to_vga>.
    Related source file is "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd".
WARNING:Xst:37 - Detected unknown constraint/property "sigis". This constraint/property is not supported by the current software release and will be ignored.
WARNING:Xst:37 - Detected unknown constraint/property "sigis". This constraint/property is not supported by the current software release and will be ignored.
WARNING:Xst:37 - Detected unknown constraint/property "sigis". This constraint/property is not supported by the current software release and will be ignored.
WARNING:Xst:37 - Detected unknown constraint/property "sigis". This constraint/property is not supported by the current software release and will be ignored.
WARNING:Xst:647 - Input <FSL_S_Clk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <FSL_S_Control> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
INFO:Xst:3210 - "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd" line 163: Output port <blank> of the instance <vga> is unconnected or connected to loadless signal.
INFO:Xst:3210 - "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\hdl\vhdl\mem_to_vga.vhd" line 163: Output port <new_frame> of the instance <vga> is unconnected or connected to loadless signal.
    Found 8-bit register for signal <fsl_count>.
    Found 9-bit register for signal <offset>.
    Found 7-bit register for signal <addr1>.
    Found 9-bit register for signal <addr2>.
    Found 1-bit register for signal <ram_we>.
    Found 4-bit register for signal <ram_din>.
    Found 32-bit register for signal <ram_offset>.
    Found 2-bit register for signal <state>.
    Found finite state machine <FSM_0> for signal <state>.
    -----------------------------------------------------------------------
    | States             | 3                                              |
    | Transitions        | 8                                              |
    | Inputs             | 4                                              |
    | Outputs            | 2                                              |
    | Clock              | FSL_Clk (rising_edge)                          |
    | Power Up State     | idle                                           |
    | Encoding           | auto                                           |
    | Implementation     | LUT                                            |
    -----------------------------------------------------------------------
    Found 32-bit adder for signal <n0101> created at line 237.
    Found 32-bit adder for signal <ram_offset[31]_GND_4_o_add_33_OUT> created at line 253.
    Found 8-bit adder for signal <fsl_count[7]_GND_4_o_add_34_OUT> created at line 256.
    Found 11-bit adder for signal <hcount[10]_GND_4_o_add_50_OUT> created at line 1241.
    Found 9-bit subtractor for signal <GND_4_o_GND_4_o_sub_21_OUT<8:0>> created at line 227.
    Found 5-bit subtractor for signal <GND_4_o_ram_offset[31]_sub_25_OUT<4:0>> created at line 239.
    Found 9-bit subtractor for signal <GND_4_o_GND_4_o_sub_52_OUT<8:0>> created at line 1308.
    Found 4-bit 29-to-1 multiplexer for signal <n0130> created at line 230.
    Found 32-bit comparator greater for signal <ram_offset[31]_GND_4_o_LessThan_23_o> created at line 235
    Found 11-bit comparator greater for signal <hcount[10]_GND_4_o_LessThan_46_o> created at line 260
    Found 11-bit comparator greater for signal <vcount[10]_GND_4_o_LessThan_47_o> created at line 260
    Found 11-bit comparator greater for signal <hcount[10]_GND_4_o_LessThan_49_o> created at line 263
    Summary:
	inferred   6 Adder/Subtractor(s).
	inferred  70 D-type flip-flop(s).
	inferred   4 Comparator(s).
	inferred  15 Multiplexer(s).
	inferred   1 Finite State Machine(s).
Unit <mem_to_vga> synthesized.

Synthesizing Unit <vga_controller_640_60>.
    Related source file is "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\devl\projnav\vga_controller_640_60.vhd".
    Found 11-bit register for signal <hcounter>.
    Found 11-bit register for signal <vcounter>.
    Found 1-bit register for signal <HS>.
    Found 1-bit register for signal <VS>.
    Found 1-bit register for signal <blank>.
    Found 11-bit adder for signal <hcounter[10]_GND_8_o_add_4_OUT> created at line 164.
    Found 11-bit adder for signal <vcounter[10]_GND_8_o_add_10_OUT> created at line 181.
    Found 11-bit comparator greater for signal <n0004> created at line 147
    Found 11-bit comparator lessequal for signal <n0017> created at line 194
    Found 11-bit comparator greater for signal <hcounter[10]_GND_8_o_LessThan_17_o> created at line 194
    Found 11-bit comparator lessequal for signal <n0023> created at line 210
    Found 11-bit comparator greater for signal <vcounter[10]_GND_8_o_LessThan_19_o> created at line 210
    Found 11-bit comparator greater for signal <hcounter[10]_GND_8_o_LessThan_20_o> created at line 219
    Summary:
	inferred   2 Adder/Subtractor(s).
	inferred  25 D-type flip-flop(s).
	inferred   6 Comparator(s).
	inferred   2 Multiplexer(s).
Unit <vga_controller_640_60> synthesized.

Synthesizing Unit <block_ram>.
    Related source file is "C:\Temp\tupmmama\pcores\mem_to_vga_v1_00_a\devl\projnav\block_ram.vhd".
WARNING:Xst:647 - Input <addr1<31:7>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <addr2<31:9>> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_8>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_8> for signal <ram_8>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_7>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_7> for signal <ram_7>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_0>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_0> for signal <ram_0>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_2>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_2> for signal <ram_2>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_1>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_1> for signal <ram_1>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_6>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_6> for signal <ram_6>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_5>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_5> for signal <ram_5>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_4>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_4> for signal <ram_4>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_3>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_3> for signal <ram_3>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_13>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_13> for signal <ram_13>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_9>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_9> for signal <ram_9>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_10>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_10> for signal <ram_10>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_11>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_11> for signal <ram_11>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_12>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_12> for signal <ram_12>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_14>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_14> for signal <ram_14>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_15>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_15> for signal <ram_15>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_16>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_16> for signal <ram_16>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_17>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_17> for signal <ram_17>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_18>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_18> for signal <ram_18>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_19>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_19> for signal <ram_19>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_20>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_20> for signal <ram_20>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_21>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_21> for signal <ram_21>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_22>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_22> for signal <ram_22>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_23>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_23> for signal <ram_23>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_24>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_24> for signal <ram_24>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_25>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_25> for signal <ram_25>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_26>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_26> for signal <ram_26>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_27>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_27> for signal <ram_27>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_28>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_28> for signal <ram_28>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_29>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_29> for signal <ram_29>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_30>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_30> for signal <ram_30>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_31>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_31> for signal <ram_31>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_32>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_32> for signal <ram_32>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_33>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_33> for signal <ram_33>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_34>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_34> for signal <ram_34>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_35>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_35> for signal <ram_35>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_36>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_36> for signal <ram_36>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_37>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_37> for signal <ram_37>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_38>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_38> for signal <ram_38>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_39>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_39> for signal <ram_39>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_40>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_40> for signal <ram_40>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_41>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_41> for signal <ram_41>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_42>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_42> for signal <ram_42>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_43>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_43> for signal <ram_43>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_44>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_44> for signal <ram_44>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_45>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_45> for signal <ram_45>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_46>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_46> for signal <ram_46>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_47>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_47> for signal <ram_47>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_48>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_48> for signal <ram_48>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_49>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_49> for signal <ram_49>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_50>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_50> for signal <ram_50>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_51>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_51> for signal <ram_51>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_52>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_52> for signal <ram_52>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_53>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_53> for signal <ram_53>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_54>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_54> for signal <ram_54>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_55>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_55> for signal <ram_55>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_56>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_56> for signal <ram_56>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_57>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_57> for signal <ram_57>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_58>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_58> for signal <ram_58>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_59>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_59> for signal <ram_59>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_60>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_60> for signal <ram_60>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_61>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_61> for signal <ram_61>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_62>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_62> for signal <ram_62>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_63>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_63> for signal <ram_63>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_64>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_64> for signal <ram_64>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_65>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_65> for signal <ram_65>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_66>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_66> for signal <ram_66>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_67>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_67> for signal <ram_67>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_68>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_68> for signal <ram_68>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_69>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_69> for signal <ram_69>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_70>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_70> for signal <ram_70>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_71>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_71> for signal <ram_71>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_72>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_72> for signal <ram_72>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_73>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_73> for signal <ram_73>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_74>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_74> for signal <ram_74>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_75>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_75> for signal <ram_75>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_76>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_76> for signal <ram_76>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_77>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_77> for signal <ram_77>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_78>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_78> for signal <ram_78>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_79>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_79> for signal <ram_79>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_80>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_80> for signal <ram_80>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_81>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_81> for signal <ram_81>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_82>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_82> for signal <ram_82>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_83>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_83> for signal <ram_83>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_84>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_84> for signal <ram_84>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_85>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_85> for signal <ram_85>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_86>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_86> for signal <ram_86>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_87>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_87> for signal <ram_87>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_88>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_88> for signal <ram_88>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_89>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_89> for signal <ram_89>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_90>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_90> for signal <ram_90>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_91>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_91> for signal <ram_91>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_92>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_92> for signal <ram_92>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_93>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_93> for signal <ram_93>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_94>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_94> for signal <ram_94>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_95>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_95> for signal <ram_95>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_96>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_96> for signal <ram_96>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_97>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_97> for signal <ram_97>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_98>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_98> for signal <ram_98>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_99>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_99> for signal <ram_99>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_100>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_100> for signal <ram_100>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_101>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_101> for signal <ram_101>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_102>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_102> for signal <ram_102>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_103>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_103> for signal <ram_103>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_104>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_104> for signal <ram_104>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_105>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_105> for signal <ram_105>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_106>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_106> for signal <ram_106>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_107>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_107> for signal <ram_107>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_108>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_108> for signal <ram_108>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_109>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_109> for signal <ram_109>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_110>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_110> for signal <ram_110>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_111>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_111> for signal <ram_111>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_112>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_112> for signal <ram_112>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_113>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_113> for signal <ram_113>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_114>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_114> for signal <ram_114>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_115>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_115> for signal <ram_115>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_116>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_116> for signal <ram_116>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_117>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_117> for signal <ram_117>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_118>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_118> for signal <ram_118>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_119>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_119> for signal <ram_119>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_120>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_120> for signal <ram_120>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_121>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_121> for signal <ram_121>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_122>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_122> for signal <ram_122>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_123>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_123> for signal <ram_123>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_124>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_124> for signal <ram_124>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_125>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_125> for signal <ram_125>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_126>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_126> for signal <ram_126>.
WARNING:Xst:3035 - Index value(s) does not match array range for signal <ram_127>, simulation mismatch.
    Found 300x4-bit single-port RAM <Mram_ram_127> for signal <ram_127>.
    Found 4-bit register for signal <data_o>.
    Summary:
	inferred 128 RAM(s).
	inferred   4 D-type flip-flop(s).
Unit <block_ram> synthesized.

=========================================================================
HDL Synthesis Report

Macro Statistics
# RAMs                                                 : 128
 300x4-bit single-port RAM                             : 128
# Adders/Subtractors                                   : 8
 11-bit adder                                          : 3
 32-bit adder                                          : 2
 5-bit subtractor                                      : 1
 8-bit adder                                           : 1
 9-bit subtractor                                      : 1
# Registers                                            : 13
 1-bit register                                        : 4
 11-bit register                                       : 2
 32-bit register                                       : 1
 4-bit register                                        : 2
 7-bit register                                        : 1
 8-bit register                                        : 1
 9-bit register                                        : 2
# Comparators                                          : 10
 11-bit comparator greater                             : 7
 11-bit comparator lessequal                           : 2
 32-bit comparator greater                             : 1
# Multiplexers                                         : 17
 1-bit 2-to-1 multiplexer                              : 2
 11-bit 2-to-1 multiplexer                             : 2
 32-bit 2-to-1 multiplexer                             : 2
 4-bit 2-to-1 multiplexer                              : 1
 4-bit 29-to-1 multiplexer                             : 1
 7-bit 2-to-1 multiplexer                              : 2
 8-bit 2-to-1 multiplexer                              : 2
 9-bit 2-to-1 multiplexer                              : 5
# FSMs                                                 : 1
# Xors                                                 : 896
 1-bit xor2                                            : 896

=========================================================================
INFO:Xst:1767 - HDL ADVISOR - Resource sharing has identified that some arithmetic operations in this design can share the same physical resources for reduced device utilization. For improved clock frequency you may try to disable resource sharing.

=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================

WARNING:Xst:1293 - FF/Latch <offset_0> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_1> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_2> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_3> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_4> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_5> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_6> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_7> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_8> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.

Synthesizing (advanced) Unit <mem_to_vga>.
The following registers are absorbed into accumulator <fsl_count>: 1 register on signal <fsl_count>.
INFO:Xst:3230 - The RAM description <ram/Mram_ram_127> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_126> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_125> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_124> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_123> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_122> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_121> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_120> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_119> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_118> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_117> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_116> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_115> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_114> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_113> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_112> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_111> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_110> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_109> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_108> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_107> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_106> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_105> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_104> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_103> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_102> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_101> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_100> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_99> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_97> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_98> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_96> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_95> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_94> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_93> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_92> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_91> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_90> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_89> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_88> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_87> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_86> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_85> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_84> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_83> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_82> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_81> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_80> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_79> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_78> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_77> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_76> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_75> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_74> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_73> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_72> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_71> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_70> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_69> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_68> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_67> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_66> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_64> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_65> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_63> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_62> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_61> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_60> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_59> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_58> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_57> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_56> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_55> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_54> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_53> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_52> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_51> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_50> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_49> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_48> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_47> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_46> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_45> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_44> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_43> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_42> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_41> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_40> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_39> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_38> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_37> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_36> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_35> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_34> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_33> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_31> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_32> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_30> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_29> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_28> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_27> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_26> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_25> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_24> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_23> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_22> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_21> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_20> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_19> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_18> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_17> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_16> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_15> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_14> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_12> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_11> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_10> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_9> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_13> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_3> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_4> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_5> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_6> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_1> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_2> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_0> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3230 - The RAM description <ram/Mram_ram_7> will not be implemented on the device block RAM because of limited available resources. If you would like this RAM to be implemented in block RAM, please select a larger device or increase the value specified by the BRAM_Utilization_Ratio constraint.
    -----------------------------------------------------------------------
    | ram_type           | Distributed                         |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    |     doA            | connected to internal node          |          |
    -----------------------------------------------------------------------
INFO:Xst:3225 - The RAM <ram/Mram_ram_8> will be implemented as BLOCK RAM
    -----------------------------------------------------------------------
    | ram_type           | Block                               |          |
    -----------------------------------------------------------------------
    | Port A                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkA           | connected to signal <FSL_Clk>       | rise     |
    |     weA            | connected to internal node          | high     |
    |     addrA          | connected to signal <addr2>         |          |
    |     diA            | connected to signal <ram_din>       |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
    | Port B                                                              |
    |     aspect ratio   | 300-word x 4-bit                    |          |
    |     mode           | write-first                         |          |
    |     clkB           | connected to signal <FSL_Clk>       | rise     |
    |     addrB          | connected to signal <naddr2>        |          |
    |     doB            | connected to internal node          |          |
    -----------------------------------------------------------------------
    | optimization       | speed                               |          |
    -----------------------------------------------------------------------
Unit <mem_to_vga> synthesized (advanced).

Synthesizing (advanced) Unit <vga_controller_640_60>.
The following registers are absorbed into counter <hcounter>: 1 register on signal <hcounter>.
The following registers are absorbed into counter <vcounter>: 1 register on signal <vcounter>.
Unit <vga_controller_640_60> synthesized (advanced).

=========================================================================
Advanced HDL Synthesis Report

Macro Statistics
# RAMs                                                 : 128
 300x4-bit dual-port block RAM                         : 32
 300x4-bit single-port distributed RAM                 : 96
# Adders/Subtractors                                   : 5
 11-bit adder                                          : 1
 32-bit adder                                          : 1
 5-bit subtractor                                      : 1
 7-bit adder                                           : 1
 9-bit subtractor                                      : 1
# Counters                                             : 2
 11-bit up counter                                     : 2
# Accumulators                                         : 1
 8-bit up accumulator                                  : 1
# Registers                                            : 69
 Flip-Flops                                            : 69
# Comparators                                          : 10
 11-bit comparator greater                             : 7
 11-bit comparator lessequal                           : 2
 32-bit comparator greater                             : 1
# Multiplexers                                         : 15
 1-bit 2-to-1 multiplexer                              : 2
 32-bit 2-to-1 multiplexer                             : 2
 4-bit 2-to-1 multiplexer                              : 1
 4-bit 29-to-1 multiplexer                             : 1
 7-bit 2-to-1 multiplexer                              : 2
 8-bit 2-to-1 multiplexer                              : 2
 9-bit 2-to-1 multiplexer                              : 5
# FSMs                                                 : 1
# Xors                                                 : 896
 1-bit xor2                                            : 896

=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================
WARNING:Xst:1293 - FF/Latch <offset_0> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_1> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_2> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_3> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_4> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_5> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_6> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_7> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <offset_8> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
Analyzing FSM <MFsm> for best encoding.
Optimizing FSM <FSM_0> on signal <state[1:2]> with gray encoding.
----------------------
 State    | Encoding
----------------------
 idle     | 00
 read_fsl | 11
 resp_px  | 01
----------------------
WARNING:Xst:1293 - FF/Latch <fsl_count_0> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <fsl_count_1> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <fsl_count_2> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:2677 - Node <fsl_count_7> of sequential type is unconnected in block <mem_to_vga>.

Optimizing unit <mem_to_vga> ...
WARNING:Xst:1293 - FF/Latch <ram_offset_0> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.
WARNING:Xst:1896 - Due to other FF/Latch trimming, FF/Latch <ram_offset_1> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.

Optimizing unit <vga_controller_640_60> ...
WARNING:Xst:2677 - Node <vga/blank> of sequential type is unconnected in block <mem_to_vga>.
WARNING:Xst:1293 - FF/Latch <vga/hcounter_10> has a constant value of 0 in block <mem_to_vga>. This FF/Latch will be trimmed during the optimization process.

Mapping all equations...
Building and optimizing final netlist ...
Found area constraint ratio of 100 (+ 5) on block mem_to_vga, actual ratio is 13.
FlipFlop addr1_2 has been replicated 8 time(s)
FlipFlop addr1_3 has been replicated 7 time(s)
FlipFlop addr1_4 has been replicated 7 time(s)
FlipFlop addr1_5 has been replicated 7 time(s)
FlipFlop addr1_6 has been replicated 7 time(s)
FlipFlop addr2_0 has been replicated 15 time(s)
FlipFlop addr2_1 has been replicated 15 time(s)
FlipFlop addr2_2 has been replicated 14 time(s)
FlipFlop addr2_3 has been replicated 14 time(s)
FlipFlop addr2_4 has been replicated 14 time(s)
FlipFlop addr2_5 has been replicated 14 time(s)

Final Macro Processing ...

=========================================================================
Final Register Report

Macro Statistics
# Registers                                            : 206
 Flip-Flops                                            : 206

=========================================================================

=========================================================================
*                           Partition Report                            *
=========================================================================

Partition Implementation Status
-------------------------------

  No Partitions were found in this design.

-------------------------------

=========================================================================
*                            Design Summary                             *
=========================================================================

Top Level Output File Name         : mem_to_vga.ngc

Primitive and Black Box Usage:
------------------------------
# BELS                             : 1198
#      GND                         : 1
#      INV                         : 4
#      LUT1                        : 30
#      LUT2                        : 221
#      LUT3                        : 50
#      LUT4                        : 55
#      LUT5                        : 69
#      LUT6                        : 651
#      MUXCY                       : 60
#      VCC                         : 1
#      XORCY                       : 56
# FlipFlops/Latches                : 206
#      FD                          : 6
#      FDE                         : 176
#      FDR                         : 12
#      FDRE                        : 12
# RAMS                             : 800
#      RAM256X1S                   : 384
#      RAM64X1S                    : 384
#      RAMB8BWER                   : 32
# Clock Buffers                    : 2
#      BUFGP                       : 2
# IO Buffers                       : 45
#      IBUF                        : 34
#      OBUF                        : 11

Device utilization summary:
---------------------------

Selected Device : 6slx16csg324-2 


Slice Logic Utilization: 
 Number of Slice Registers:             206  out of  18224     1%  
 Number of Slice LUTs:                 3000  out of   9112    32%  
    Number used as Logic:              1080  out of   9112    11%  
    Number used as Memory:             1920  out of   2176    88%  
       Number used as RAM:             1920

Slice Logic Distribution: 
 Number of LUT Flip Flop pairs used:   3079
   Number with an unused Flip Flop:    2873  out of   3079    93%  
   Number with an unused LUT:            79  out of   3079     2%  
   Number of fully used LUT-FF pairs:   127  out of   3079     4%  
   Number of unique control sets:         9

IO Utilization: 
 Number of IOs:                          49
 Number of bonded IOBs:                  47  out of    232    20%  

Specific Feature Utilization:
 Number of Block RAM/FIFO:               16  out of     32    50%  
    Number using Block RAM only:         16
 Number of BUFG/BUFGCTRLs:                2  out of     16    12%  

---------------------------
Partition Resource Summary:
---------------------------

  No Partitions were found in this design.

---------------------------


=========================================================================
Timing Report

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.
      FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT
      GENERATED AFTER PLACE-and-ROUTE.

Clock Information:
------------------
-----------------------------------+------------------------+-------+
Clock Signal                       | Clock buffer(FF name)  | Load  |
-----------------------------------+------------------------+-------+
FSL_Clk                            | BUFGP                  | 983   |
pixel_clk                          | BUFGP                  | 23    |
-----------------------------------+------------------------+-------+

Asynchronous Control Signals Information:
----------------------------------------
No asynchronous control signals found in this design

Timing Summary:
---------------
Speed Grade: -2

   Minimum period: 8.537ns (Maximum Frequency: 117.137MHz)
   Minimum input arrival time before clock: 7.359ns
   Maximum output required time after clock: 9.898ns
   Maximum combinational path delay: 6.016ns

Timing Details:
---------------
All values displayed in nanoseconds (ns)

=========================================================================
Timing constraint: Default period analysis for Clock 'FSL_Clk'
  Clock period: 8.537ns (frequency: 117.137MHz)
  Total number of paths / destination ports: 44099 / 8040
-------------------------------------------------------------------------
Delay:               8.537ns (Levels of Logic = 6)
  Source:            addr1_0 (FF)
  Destination:       ram/data_o_0 (FF)
  Source Clock:      FSL_Clk rising
  Destination Clock: FSL_Clk rising

  Data Path: addr1_0 to ram/data_o_0
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDE:C->Q             18   0.525   1.343  addr1_0 (addr1_0)
     LUT2:I0->O           19   0.250   1.261  ram/PWR_14_o_GND_59_o_OR_2083_o_SW0_1 (ram/PWR_14_o_GND_59_o_OR_2083_o_SW0)
     LUT6:I5->O            4   0.254   0.912  ram/PWR_14_o_GND_59_o_OR_1683_o (ram/PWR_14_o_GND_59_o_OR_1683_o)
     LUT6:I4->O            1   0.250   1.112  ram/addr1[6]_read_port_1_OUT<0>13 (ram/addr1[6]_read_port_1_OUT<0>13)
     LUT6:I1->O            1   0.254   0.682  ram/addr1[6]_read_port_1_OUT<0>14_SW0 (N2006)
     LUT6:I5->O            1   0.254   1.112  ram/addr1[6]_read_port_1_OUT<0>14 (ram/addr1[6]_read_port_1_OUT<0>14)
     LUT6:I1->O            1   0.254   0.000  ram/addr1[6]_read_port_1_OUT<0>97 (ram/addr1[6]_read_port_1_OUT<0>)
     FD:D                      0.074          ram/data_o_0
    ----------------------------------------
    Total                      8.537ns (2.115ns logic, 6.422ns route)
                                       (24.8% logic, 75.2% route)

=========================================================================
Timing constraint: Default period analysis for Clock 'pixel_clk'
  Clock period: 5.691ns (frequency: 175.716MHz)
  Total number of paths / destination ports: 1744 / 34
-------------------------------------------------------------------------
Delay:               5.691ns (Levels of Logic = 13)
  Source:            vga/hcounter_4 (FF)
  Destination:       vga/hcounter_9 (FF)
  Source Clock:      pixel_clk rising
  Destination Clock: pixel_clk rising

  Data Path: vga/hcounter_4 to vga/hcounter_9
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDR:C->Q              8   0.525   1.374  vga/hcounter_4 (vga/hcounter_4)
     LUT5:I0->O            2   0.254   0.834  vga/hcounter[10]_GND_8_o_equal_4_o<10>_SW0 (N2000)
     LUT6:I4->O           21   0.250   1.538  vga/hcounter[10]_GND_8_o_equal_4_o<10> (vga/hcounter[10]_GND_8_o_equal_4_o)
     LUT3:I0->O            1   0.235   0.000  vga/Mcount_hcounter_lut<0> (vga/Mcount_hcounter_lut<0>)
     MUXCY:S->O            1   0.215   0.000  vga/Mcount_hcounter_cy<0> (vga/Mcount_hcounter_cy<0>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<1> (vga/Mcount_hcounter_cy<1>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<2> (vga/Mcount_hcounter_cy<2>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<3> (vga/Mcount_hcounter_cy<3>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<4> (vga/Mcount_hcounter_cy<4>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<5> (vga/Mcount_hcounter_cy<5>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<6> (vga/Mcount_hcounter_cy<6>)
     MUXCY:CI->O           1   0.023   0.000  vga/Mcount_hcounter_cy<7> (vga/Mcount_hcounter_cy<7>)
     MUXCY:CI->O           0   0.023   0.000  vga/Mcount_hcounter_cy<8> (vga/Mcount_hcounter_cy<8>)
     XORCY:CI->O           1   0.206   0.000  vga/Mcount_hcounter_xor<9> (vga/Mcount_hcounter9)
     FDR:D                     0.074          vga/hcounter_9
    ----------------------------------------
    Total                      5.691ns (1.945ns logic, 3.746ns route)
                                       (34.2% logic, 65.8% route)

=========================================================================
Timing constraint: Default OFFSET IN BEFORE for Clock 'FSL_Clk'
  Total number of paths / destination ports: 964 / 472
-------------------------------------------------------------------------
Offset:              7.359ns (Levels of Logic = 4)
  Source:            FSL_Rst (PAD)
  Destination:       ram/Mram_ram_99 (RAM)
  Destination Clock: FSL_Clk rising

  Data Path: FSL_Rst to ram/Mram_ram_99
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     IBUF:I->O            29   1.328   1.746  FSL_Rst_IBUF (FSL_Rst_IBUF)
     LUT4:I0->O            1   0.254   0.000  _n01941_lut1 (_n01941_lut1)
     MUXCY:S->O            9   0.427   1.431  _n01941_cy1 (_n0194)
     LUT6:I0->O           32   0.254   1.519  naddr2<3>_0_01 (naddr2<3>_0_0)
     RAMB8BWER:ADDRBRDADDR5        0.400          ram/Mram_ram_99
    ----------------------------------------
    Total                      7.359ns (2.663ns logic, 4.696ns route)
                                       (36.2% logic, 63.8% route)

=========================================================================
Timing constraint: Default OFFSET IN BEFORE for Clock 'pixel_clk'
  Total number of paths / destination ports: 21 / 21
-------------------------------------------------------------------------
Offset:              3.256ns (Levels of Logic = 1)
  Source:            FSL_Rst (PAD)
  Destination:       vga/vcounter_10 (FF)
  Destination Clock: pixel_clk rising

  Data Path: FSL_Rst to vga/vcounter_10
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     IBUF:I->O            29   1.328   1.469  FSL_Rst_IBUF (FSL_Rst_IBUF)
     FDR:R                     0.459          vga/hcounter_0
    ----------------------------------------
    Total                      3.256ns (1.787ns logic, 1.469ns route)
                                       (54.9% logic, 45.1% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'FSL_Clk'
  Total number of paths / destination ports: 48 / 7
-------------------------------------------------------------------------
Offset:              8.129ns (Levels of Logic = 10)
  Source:            ram_offset_3 (FF)
  Destination:       FSL_S_Read (PAD)
  Source Clock:      FSL_Clk rising

  Data Path: ram_offset_3 to FSL_S_Read
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDE:C->Q             13   0.525   1.206  ram_offset_3 (ram_offset_3)
     LUT3:I1->O            1   0.250   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_lut<0>1 (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_lut<0>)
     MUXCY:S->O            1   0.215   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<0> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<0>)
     MUXCY:CI->O           1   0.023   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<1> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<1>)
     MUXCY:CI->O           1   0.023   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<2> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<2>)
     MUXCY:CI->O           1   0.023   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<3> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<3>)
     MUXCY:CI->O           1   0.023   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<4> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<4>)
     MUXCY:CI->O           1   0.023   0.000  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<5> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<5>)
     MUXCY:CI->O          45   0.023   1.965  Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<6> (Mcompar_ram_offset[31]_GND_4_o_LessThan_23_o_cy<6>)
     LUT3:I0->O            1   0.235   0.681  _n0178_inv11 (FSL_S_Read_OBUF)
     OBUF:I->O                 2.912          FSL_S_Read_OBUF (FSL_S_Read)
    ----------------------------------------
    Total                      8.129ns (4.277ns logic, 3.852ns route)
                                       (52.6% logic, 47.4% route)

=========================================================================
Timing constraint: Default OFFSET OUT AFTER for Clock 'pixel_clk'
  Total number of paths / destination ports: 74 / 8
-------------------------------------------------------------------------
Offset:              9.898ns (Levels of Logic = 5)
  Source:            vga/hcounter_4 (FF)
  Destination:       rgb<1> (PAD)
  Source Clock:      pixel_clk rising

  Data Path: vga/hcounter_4 to rgb<1>
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDR:C->Q              8   0.525   1.172  vga/hcounter_4 (vga/hcounter_4)
     LUT3:I0->O            2   0.235   0.954  hcount[10]_GND_4_o_LessThan_46_o1_SW0 (N1992)
     LUT6:I3->O           14   0.235   1.557  hcount[10]_GND_4_o_LessThan_46_o1 (hcount[10]_GND_4_o_LessThan_46_o)
     LUT5:I0->O            7   0.254   1.138  hcount[10]_vcount[10]_AND_12_o1 (hcount[10]_vcount[10]_AND_12_o)
     LUT4:I1->O            1   0.235   0.681  Mmux_rgb21 (rgb_1_OBUF)
     OBUF:I->O                 2.912          rgb_1_OBUF (rgb<1>)
    ----------------------------------------
    Total                      9.898ns (4.396ns logic, 5.502ns route)
                                       (44.4% logic, 55.6% route)

=========================================================================
Timing constraint: Default path analysis
  Total number of paths / destination ports: 1 / 1
-------------------------------------------------------------------------
Delay:               6.016ns (Levels of Logic = 3)
  Source:            FSL_S_Exists (PAD)
  Destination:       FSL_S_Read (PAD)

  Data Path: FSL_S_Exists to FSL_S_Read
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     IBUF:I->O             5   1.328   0.841  FSL_S_Exists_IBUF (FSL_S_Exists_IBUF)
     LUT3:I2->O            1   0.254   0.681  _n0178_inv11 (FSL_S_Read_OBUF)
     OBUF:I->O                 2.912          FSL_S_Read_OBUF (FSL_S_Read)
    ----------------------------------------
    Total                      6.016ns (4.494ns logic, 1.522ns route)
                                       (74.7% logic, 25.3% route)

=========================================================================

Cross Clock Domains Report:
--------------------------

Clock to Setup on destination clock FSL_Clk
---------------+---------+---------+---------+---------+
               | Src:Rise| Src:Fall| Src:Rise| Src:Fall|
Source Clock   |Dest:Rise|Dest:Rise|Dest:Fall|Dest:Fall|
---------------+---------+---------+---------+---------+
FSL_Clk        |    8.537|         |         |         |
pixel_clk      |   10.336|         |         |         |
---------------+---------+---------+---------+---------+

Clock to Setup on destination clock pixel_clk
---------------+---------+---------+---------+---------+
               | Src:Rise| Src:Fall| Src:Rise| Src:Fall|
Source Clock   |Dest:Rise|Dest:Rise|Dest:Fall|Dest:Fall|
---------------+---------+---------+---------+---------+
pixel_clk      |    5.691|         |         |         |
---------------+---------+---------+---------+---------+

=========================================================================


Total REAL time to Xst completion: 21.00 secs
Total CPU time to Xst completion: 21.49 secs
 
--> 

Total memory usage is 285084 kilobytes

Number of errors   :    0 (   0 filtered)
Number of warnings :  162 (   0 filtered)
Number of infos    :  131 (   0 filtered)

